Vicon® Industries IQaccess Remote Video Monitoring Software
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE
PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	General Software Description 
The specified product is an on-camera intelligent software for IQeye Alliance-mx, Alliance-mini and 7 Series cameras that shall enable multiple users to receive alerts via a pop-up video window when the camera receives an internal or external trigger. The first responder then has the option to activate a relay and/or signal a third party device via TCP/IP. For IQeye cameras that have audio, the user can also receive audio from an external microphone attached to the camera and push-to-talk back to a camera with an audio output. 

2.03	General Software Requirements
A.	The product shall allow up to 8 local or remote users to register with each IQaccess enabled IQeye camera.

B. The product shall not require a browser to operate.

C. The product shall be configurable to automatically launch whenever the PC starts.

D. The product shall be configurable to a talk mode using the push-to-talk button in the alert pop-up window generated by the camera.  

E. The product shall be configurable to a listen mode only from the camera that generated the alert pop-up window.  

F. The product shall be configurable for both talk and listen modes from the camera that generates the alert pop-up window.

G. The product shall automatically search the network and identify any IQaccess enabled camera on the same subnet.

H. The product shall allow users to register their PC with any/all IQaccess enabled cameras provided they have the appropriate credentials.

I. The product shall allow remote users to register with the IQaccess enabled cameras via direct connection or a Port Forwarded Address.

J. The product shall allow users with administrative credentials to disable selected users from accessing the IQaccess enabled cameras.

K. The product shall be configured so relay activation and/or third party systems will require a password for each activation control.

L. The product shall allow users to elect to receive alerts 24/7 or within the scheduled hours when registering a PC with IQaccess.

M. The product shall allow administrators to choose the name of the relay trigger button that appears in the alert screen.

N. The product shall deliver video using MJPEG compression at VGA resolution 640 x 480 up to 2 frames per second (fps).

2.04	PC Requirements:
A.	Windows XP or Vista operating systems

B. Intel Pentium 4 or above CPU

C. Minimum of 512MB of RAM 

D. 50GB Hard Drive	

E. 10/100-BaseT network interface

2.05	Approved Manufacturers:
The Remote Video Monitoring Software shall be Vicon Industries model IQaccess.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.