Vicon® Industries V2000-WIR-360 SERIES MULTI-SENSOR CAMERAS 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR MULTI-SENSOR SERIES CAMERA 

A.	The outdoor multi-sensor camera shall incorporate four camera/lens modules to provide a 360° panoramic view. The camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall have true WDR and IR capability and include four integral motorized lenses. Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 131 ft (40 m). A clear polycarbonate lower dome shall be included. Starlight low-light imaging shall be provided by these cameras.

B.	All four sensors shall be motorized so users can quickly and easily configure them remotely. The cameras shall include presets for 180°, 270° and 360° of coverage; customized views shall also be configurable through each sensor’s PTZ controls.

C.	The camera shall have smart encoding, which monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.

D.	The camera shall be powered by PoE++, 24 VAC or 24 VDC. 

E.	The camera shall have triple streaming video and support H.264/H.265 compression. The camera modules shall be available in 5 MP or 8 MP resolution, offering a 20 MP or 32 MP resolution mode. 

F.	Camera features shall include electronic iris, AGC, true WDR, white balance, backlight compensation, tampering, flip, mirror, privacy masks and motion detection.

G.	The camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals.

H.	The camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface. It shall be IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance. The camera shall be NDAA compliant.

I.	The camera shall provide a slot for an SD card for local storage.

J.	There shall be mounting accessories to allow wall mounting, pendant mounting, and an adapter to allow corner and pole mounting.

K.	The fixed-position camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP CAMERA DOME SPECIFICATIONS

A.	Imaging Device:	5 MP: 4x 1/2.8-inch progressive scan CMOS 
          	8MP: 4x 1/1.8-inch progressive scan CMOS
	
B.	Max. Resolution:	4x 2592 x 1944 (5 MP)
                                             4x 3840 x 2160 (8 MP)
C.	Shutter Speed:	1/7 - 1/20,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity:	20 MP: Color: 0.03 lux; B&W: 0.01 (IR OFF), 0 lux (IR On) @30 IRE
32 MP: Color: 0.02 lux; B&W: 0.01 (IR OFF), 0 lux (IR On) @30 IRE

F.	Wide Dynamic Range	True WDR, 120dB
G.	Focal Length:	4x 3.1-10 mm
H.	Field of View (tele-wide):	20 MP: Horiz: 32°-96°; Vert: 24°-69°; Depth: 40°-124° 
                                             32 MP: Horiz: 46°-98°; Vert: 26°-54°; Depth: 54°-113°
I.	IR Distance:	131 ft (40 m) @ IEEE802.3bt

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE++ (IEEE802.3bt Class 5), 24 VAC, 24 VDC 
B.	Current (IR on):	1.7 A; 
                                              
C.	Power Consumption 
(IR on):	40 W
D.	Connectors:	Pigtail: Power: terminal block 
	PoE/Network: RJ-45
		Alarm In/Out: terminal block
		Audio: phone jack
		Slot for SD card
		
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 131°F (-40° to 55°C) 

B.	Humidity:	10% to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Die-cast aluminum housing
Dome: clear polycarbonate
B.	Dimensions:	Height: 5.6 in. (142.3 mm), 
Diameter: 9.7 in. (247.5 mm)
C.	Weight: 	Approximately 5.2 lb (2.36 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount; includes mounting cap. Mounting options available.
B.	Remote Adjustment:	Pan 360°; Tilt: 90° (default value 83°) 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management Systems 
B.	Compression:	H.264/H.265 
C.	LAN Interface:	10/100 
D.	Video Channels	Triple streaming
E.	Max Resolution and 
Frame Rate:		20 MP: 4x 2592x1944; 32 MP: 3840 x 2160
Max 30 fps at 20 MP and 32 MP
F.	Web Browser:	Internet Explorer, Firefox, Google Chrome
G.	Users:	Up to 10 clients
H.	Image Settings:	Day/night mode; flip and mirror; configurable 
                                             brightness, contrast, hue, sharpness, saturation; white 
                                             balance, gain control; DNR; true WDR (120dB); privacy 
	masks (5); motion detection; BLC; Exposure; Audio
I.	Intelligent Video Analytics:	Tampering, Intelligent Motion Detection, Intrusion 
                                             Detection; Line Cross, Loitering, Object 
                                             Left/Removed, Tailgating, Crowding.
                                             It shall also provide AI-based object classification
                                            analytics for vehicles, people and animals. This shall 
                                            enhance working with Museum Search in Valerus VMS.
J.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTP, RTCP
                                             SMTP, FTP, UDP, uPnP, QoS, ICMP, SNMP v2c/v3, 
                                             SSL, DNS, NTP, LDAP (client), Zeroconfig, DynDNS, 
                                             ONVIF S/G/M/T

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	IP66
D.	IK10
E.	UL
F.	ONVIF S/G/M/T
G.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor color IP multi-sensor camera shall be Vicon Industries Model V2020-WIR-360 (20 MP) and V2032-WIR-360 (32 MP).

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.