Vicon® Industries V2008-W-NL IP BOX CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	IP BOX CAMERA 

A.	The indoor box camera shall lightweight and compact, enabling it to be mounted in a variety of locations. The high-resolution day/night camera be available in 8 MP resolution and shall have true WDR. Day/night operation shall be achieved using a built-in IR-cut filter. 

B.	The camera shall support megapixel DC iris, P-iris or i-CS lenses. 

C.	The box camera shall be powered by PoE, 24 VAC or 12 VDC. 

D.	The box camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

E.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.

F.	The camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals.

G.	The box camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/M interface. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

H.	The box camera shall provide a slot for an SD card for local storage.

I.	The box camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP BOX CAMERA SPECIFICATIONS

A.	Imaging Device:	1/1.8-inch progressive scan 
B.	Max. Resolution:	8 MP model
C.	Shutter Speed:	1/2 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity (@ 30 IRE):	Color: 0.02 lux; B&W: 0.01 lux
F.	Tilt and Horizontal	Mount dependent 
G.	Digital Zoom:	Dynamic ROI
H.	Lens Support: 	Supports megapixel DC iris, P-iris or i-CS lenses; 
                                             auto back focus (ABF) button for easy focus adjustment

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC, 24 VAC or PoE
B.	Current:	PoE 350 mA; 12 VDC: 1. A; 24 VAC: 1 A (50/60 Hz)
C.	Power Consumption:	13.5 W 
D.	Connectors:	Power: 24 VAC/12 VDC terminal block
	PoE Power: RJ-45
		Video/Data: RJ-45
		Audio Input/Output: terminal block; audio level alarm alert
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	14° to 131°F (-10° to 55°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum alloy body; bracket: PC+ABS
B.	Dimensions:	Length: 4.1 in. (104 mm), 
Width: 2.9 in. (73 mm)
Height: 2.4 in. (62 mm)
C.	Weight: 	1.3 lb (0.8 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Screw hole provided, top and bottom, for standard mounts. 
B.	Adjustments:	Mount dependent; ¼-20 mounting hole top and bottom 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate: 8 MP: 3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             dynamic ROI
I.	Intelligent Video Analytics:	Tampering, Intelligent Motion Detection, Intrusion 
                                             Detection; Line Cross, Loitering, Object 
                                             Left/Removed, Tailgating, Crowding.
                                             It shall also provide AI-based object classification
                                            analytics for vehicles, people and animals. This shall 
                                            enhance working with Museum Search in Valerus VMS.
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/M/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	ONVIF S/T/G/M
E.	RoHS
F.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The indoor IP box camera shall be Vicon Industries V2008-W-NL.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.