Vicon® Industries V2000D OUTDOOR IP MICRO DOME CAMERA WITH BUILT IN MICROPHONE
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP DOME CAMERA 

A.	The outdoor fixed dome camera shall incorporate a fixed camera/lens combination. The camera dome shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera be available in a 5 MP resolution model and shall have true WDR and Smart IR/Adaptive IR capability and shall include an integral fixed 2.8 mm lens. Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 49 ft (15 m) with 8 IR LEDs. The camera shall have bi-directional audio, built-in mic and line out.

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation (roll), for any angle of view required. A variety of mounting options shall be available. 

C.	The camera shall provide Intelligent Video Analytics, tampering, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting, and Museum Search. The camera shall provide AI-based object classification analytics for vehicles, people and animals.

D.	The dome camera shall be powered by PoE. 

E.	The dome camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

F.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, motion detection and museum search.

G.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

H.	The dome camera shall provide a slot for an SD card for local storage.

I.	The dome camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP DOME CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.8-inch progressive scan 
B.	Max. Resolution:	5 MP model
C.	Shutter Speed:	1/2 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity (@ 30IRE):	Color: 0.03 lux; B&W: 0.01 lux/0 lux (IR Off/On)
F.	Tilt and Horizontal	Three-direction adjustment, allowing for adjustment of 
                                              pan, tilt and lens rotation (roll)
G.	Digital Zoom:	Yes (ROI)
H.	Lens Adjustment:	Fixed
I.	Focal Length:	2.8 mm 
J.	Horizontal Field of View:	104°;
K.	Vertical Field of View:	5 MP: 78°
L.	Depth Field of View:	134°
M.	IR Distance:	Smart IR/Adaptive IR; 49 ft (15 m) with 8 IR LEDs

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE
B.	Current:	PoE: 0.28 A 
C.	Power Consumption:	IR On: PoE: 13.5 W; IR Off: 8.5 W
D.	Connectors:	Pigtail cable provided; optional backbox required for
                                             cabling 
                                             PoE Power: RJ-45
		Video/Data: RJ-45
		Audio: Built-in mic; line out screw terminal; audio level alarm alert
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-22° to 131°F (-30° to 55°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum dome housing; polycarbonate clear dome
B.	Dimensions:	Height: 2.2 in. (57 mm), 
Diameter: 4.3 in. (110 mm)
C.	Weight: 	1.65 lb (0.75 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3-axis camera adjustment: pan 0°-180°; tilt 0°-80°; 
roll ±355° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate: 5 MP: 2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180
Max 30 fps 
F.	Web Browser:	Safari, Firefox, Chrome, Microsoft Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:	Tampering/Defocus, Intelligent Motion Detection 
                                             Intrusion Detection; Line Counter/Cross, Loitering, 
                                             Object Left/Removed, Wrong Direction, Area Counting.
                                            The camera shall provide AI-based object 
                                            classification analytics for vehicles, people and animals. 
                                            This shall enhance working with Museum Search in 
                                            Valerus VMS.
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/Q/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP67
E.	IK10
F.	ONVIF S/T/G/Q
G.	RoHS
H.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP micro dome camera shall be Vicon Industries V2005D-W28IRM.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.