Vicon® Industries V2005CNR-W24IR CORNER-MOUNTED CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	CORNER-MOUNTED CAMERA 

A.	The indoor high-security camera shall incorporate a housing, camera, lens and IR illuminators; the brightness of the IR illuminators shall be adjustable. Its design shall be specifically for use in corner installations such as elevators. The high-resolution 
5 MP day/night camera shall be available with an integral 2.4 mm fixed wide angle lens.

B.	The camera enclosure shall be waterproof and shall fit into a 90° corner. It shall consist of a two part aluminum, a fixed mounting frame and a removable front plate; once installed into the corner, the housing shall be ligature proof. The front plate shall be recessed and secured to the fixed frame with security screws. The front plate shall have two windows to protect the camera (6 mm thick) and IR LED illuminators (5 mm thick). 

C.	The camera shall support proprietary H.264, MPEG-4 and M-JPEG compression.

D.	The camera shall have an adjustable mount that shall allow it to be tilted up or down for an exact view.

E.	The camera shall be powered by PoE+, 24 VAC or 12 VDC.

F.	The camera shall provide alarms and audio. Privacy masks shall be available. A micro SD card slot shall be provided for local recording.

G.	The camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals.

H.	The camera shall meet the FCC requirements for a Class B device. It shall include support for the industry-standard ONVIF S/T/G/M interface. It shall be IK10- rated for impact resistance. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

I.	The camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.8-inch progressive scan RGB CMOS 
B.	Maximum Resolution:	5 MP 
C.	Camera Type:	True day/night (IR cut filter)
D.	Sensitivity:	Color: 0.00262 lux; B&W: 0.0 lux (IR On)
E.	IR Distance:	98 ft (30 m) with programmable intensity
F.	Lens:	Focal Length: 2.4 mm, fixed
Aperture: f/2.1 max
Horizontal Field-of-View: 121°
Vertical Field-of-View: 93°

2.04	NETWORK VIDEO TRANSMISSION

A.	Compression:	H.264, MPEG-4 or M-JPEG
B.	Video Streams:	10 concurrent streams max.
C.	Video Resolution:	2592x1944 (5 MP), 2688x1520, 2048x1536 (3 MP), 
                                             1920x1080 (Full HD 1080P), 1280x960 
                                             (SXVGA),1280x720 (HD 720P), 	800x600, 640x480 
                                             (VGA), 640x360, 320x240 (QVGA)
D.	Frame Rate:	Max 30 fps 
E.	Video Bandwidth:	10/100 Mbps
F.	Streaming:	Triple
G.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             dynamic ROI
H.	Intelligent Video Analytics:	Tampering, Intelligent Motion Detection, Intrusion 
                                             Detection; Line Cross, Loitering, Object 
                                             Left/Removed, Tailgating, Crowding.
                                             It shall also provide AI-based object classification
                                            analytics for vehicles, people and animals. This shall 
                                            enhance working with Museum Search in Valerus VMS.

2.05	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	24 VAC, 12 VDC or PoE+ (IEEE 802.3af Class 3)
B.	Power Consumption (IR on)	Max 12.9 W (IR On); 10.6 W (IR Off)
C.	Connectors:	Power: 12 VDC/24 VAC: screw terminal; PoE RJ-45;
	Alarms (In/Out): screw terminal; Audio (mic/spkr): screw 
	terminal. Reset button. Factory Default button. .Micro SD card slot (customer suppled cared; supports up to 1 TB).
D.	Radio Frequency	
	Emission Rating: 	FCC Class B

2.06	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-4° to 140°F -2(0° to 60°C) @PoE

2.07	PHYSICAL SPECIFICATIONS

A.	Application:	Indoor
B.	Construction:	Enclosure: aluminum
	Mounting frame: aluminum
	Window: polycarbonate
	IR: 5 mm thick; camera 6 mm thick
C.	Mounting:	Designed to be mounted into a 90° corner; front cover 
	secured with security screws
D.	Dimensions:	8.2 in. (208 mm) x 7.9 in. (200 mm) x 2.4 in. (60 mm)
	
E.	Weight: 	Approximately 4.4 lb (2 kg)

2.08	CERTIFICATIONS

A.	FCC, Class B
B.	CE
C.	UL/CUL 
D.	IP66; IK10
E.	ONVIF S/G/T/M
F.	NDAA-compliant

2.09	WARRANTY

A.	5 years, parts and labor

2.10	APPROVED MANUFACTURERS

A.	The corner-mount IP camera shall be Vicon Industries Model V2005CNR-W24IR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.