Vicon® Industries V2005D-PTZ NETWORK OUTDOOR PTZ DOME 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	NETWORK CAMERA DOME FEATURES

A.	The compact network dome shall be comprised of a camera/lens and pan/tilt drive in an attractive covert enclosure. It shall be available in a 5 MP version and shall have true WDR. It shall include an integral varifocal 5.2-148 mm lens (30X optical zoom). Day/night operation shall be achieved using a built-in IR-cut filter. It shall have starlight low-light imaging. IR distance shall be 492 ft (150 m) and it shall have automatic Smart IR/Adaptive IR capability. 

B.	The dome camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross/counting, loitering, object left/removed, wrong direction and area counting. It shall also provide AI-based object classification analytics for vehicles, people and animals.

C.	The dome camera shall be powered by PoE, 24 VAC or 48 VDC. It shall have a heater/blower system that maintains proper temperature in the camera housing and prevents fogging of the window.

D.	The dome camera shall have triple streaming video and provide network video transmission using either H.264/H.265 and M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity. The camera dome shall transmit high quality video across the network for remote viewing and recording and shall be configurable remotely from network digital video recorders and master workstations.

A.	Two alarm inputs shall be programmable for functional state (enabled or disabled); they shall be able to be set for Normally Open (NO) or Normally Closed (NC). The two alarm outputs shall be able to control external equipment; they shall be able to be set for Normally Open (NO) or Normally Closed (NC). An audio alert shall be available.

B.	There shall be 128 individual programmable preset positions available. Each preset shall be able to have an individual title and shall be adjustable for pan and tilt speed and manual or auto focus.

E.	There shall be four tours (patrols) available with up to 128 presets per tour. Each tour shall be able to have an individual title and shall be adjustable for pan, tilt and zoom speed and dwell time. Tours shall be able to be programmed to repeat.

F.	Pan and tilt functions shall be programmable. Maximum manual pan and tilt speeds shall be programmable. Maximum pan speed shall be 300 degrees/sec and maximum tilt speed shall be 160 degrees/sec. Pan and tilt speeds shall also be scalable to the zoom setting. The pan range shall be 360 degree continuous and tilt range shall be 195 degrees (-15 to 90 degrees).

E.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, electronic image/lens stabilization (EIS) and motion detection.

F.	The camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals.

G.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/M interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK7 rated for impact resistance. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

H.	The dome camera shall provide a slot for an SD card for local storage.

I.	The dome camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP DOME CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.8-inch progressive scan 
B.	Max. Resolution:	5 MP 
C.	Shutter Speed:	1/30 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	WDR:	True WDR (120 dB)
F.	Sensitivity (@ 30 IRE):	Starlight; Color: 0.03 lux; B&W: 0.01 lux
G.	Pan/Tilt Range:	360° continuous pan; 95° tilt (-15° to 90°)
H.	Lens:	5.2 – 148 mm, 30X optical zoom
I.	Digital Zoom:	8X
J.	Lens Adjustment:	Motorized lens, P-iris automatically adjusts to zoom 
                                              condition (manual mode)
K.	Horizontal Field of View:	58.1°-2.14° (wide-tele)
L.	Vertical Field of View:	33.8°-1.2° (wide-tele)
M.	IR Distance:	492 ft (150 m); Smart IR/Adaptive IR automatic IR 
N.	Heater/Blower System:	For low temperature operation: heater turns on at 59° F 
                                             (15° C); blower is always on

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	24 VAC (+20%/-10%), 48 VDC (±10%) or PoE++ 
B.	Current:	24 VAC: 2.5 A; 48 VDC: 1.25 A 
C.	Power Consumption:	Total 48 W. 
                                             PTZ Camera11 W; IR: Pan/Atilt Function: 12 W; 19 W; 
                                             Heater: 5,5 W; Blower: 0.9W
D.	Connectors:	Power: 48 VDC or 24 VAC terminal block; PoE: RJ-45
	Video/Data: RJ-45
		Alarm: screw terminal
		Audio: screw terminal
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 140°F (-40° to 60°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum base; polycarbonate clear dome
B.	Dimensions:	Height: 13.2 in. (336 mm), 
Diameter: 7.5 in. (190 mm)
C.	Weight: 	11.5 lb (5.2 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Mounting accessories available 
B.	Adjustments:	Pan 360° continuous; tilt: 95° (-15°-90) 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240 
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:	Tampering, Intelligent Motion Detection, Intrusion 
                                             Detection; Line Cross, Loitering, Object Left/Removed, 
                                             Tailgating, Crowding. It shall also provide AI-based 
                                             object classification analytics for vehicles, people and 
                                             animals. This shall enhance working with Museum 
                                             Search in Valerus VMS.
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/M/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP67
E.	IK07
F.	ONVIF S/T/G/M
G.	RoHS
H.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP PTZ dome camera shall be Vicon Industries V2005D-PTZ.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.