Vicon® Industries V2008-W0950-LPR CAMERA KIT WITH LICENSE PLATE RECOGINITION (LPR)
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	CAMERA KIT

A.	The LPR camera kit shall include a box camera, PoE housing with wall mount and IR illuminator module and a 9-50 mm iCS varifocal lens. A micro SD card and the LPR license shall also be included.

B.	The LPR box camera shall be lightweight and compact and shall include embedded License Plate Recognition (LPR) technology. The high-resolution day/night camera shall be available in 8 MP resolution and shall have true WDR. Day/night operation shall be achieved using a built-in IR-cut filter. 

C.	The LPR software shall allow capture, storing and searching on an unlimited number of license plates and allow examination of details such as vehicle color, make and model. Customized lists of license plates shall be able to be created to generate an alert; lists shall be able to be synchronized from one camera to other cameras on the system. On-screen alarm handling procedures shall provide step-by-step instructions for addressing alarms. License plates from over 70 countries shall be supported. The ability to search by plate shall be available. Having the LPR analytic on the edge shall allow for a standalone LPR solution for users who do not want to integrate with a compatible VMS; it shall be able to integrate with the manufacturer’s video management system to monitor events through its Alarms Management suite. When the LPR camera is used with Valerus, the powerful alarm handling procedures shall give you step-by-step instructions for proactively addressing alarms and alerts. For example, you shall be able to create multiple customized lists of “allow” license plates that are associated with executives, VIPs, etc. These plates shall generate an alert upon entry, and stakeholders shall be immediately notified and provided with a list of to-dos, like unlock certain doors, turn on lights, etc. Similarly, license plates on the “block” list shall have unique procedures that you can easily follow for threat mitigation.

D.	The box camera shall support the 9-50 mm i-CS lens with remote zoom and focus provided. 

E.	The box camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

F.	The box camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, BLC/HLC and motion detection.

G.	The box camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. License Plate Recognition (LPR) and Museum Search shall also be supported.

H.	The box camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. The camera kit shall meet the latest regulations required to be NDAA approved.

I.	The box camera shall provide a slot for an SD card for local storage, which shall be provided.

J.	The camera kit housing shall have built-in PoE management system and shall have integrated IR LEDs that shall have a maximum effective range of up to 459 ft (140 m). It shall also have a window heater and blower that permit low temperature operation of electronics to -4° F (-20° C).

K.	The camera kit shall meet or exceed the following design and performance specifications.

2.03	IP BOX CAMERA SPECIFICATIONS

A.	Imaging Device:	1/1.8-inch progressive scan 
B.	Max. Resolution:	3840x2160 (8 MP) 
C.	Shutter Speed:	Auto 1/2 - 1/10,000 sec; manual
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity (@ 30 IRE):	Color: 0.02 lux; B&W: 0.01 lux
F.	Digital Zoom:	Dynamic ROI
G.	Lens: 	1/1.8” format; CS mount; 9-50 focal length; 
                                              remote zoom and focus
                                             field-of-view: 46.1º x 26.3º (16:9)
H.	IR Distance	164-459 ft (50-140 m) range

2.04	CAMERA KIT ELECTRICAL SPECIFICATIONS

A.	Power Input:	60 W/90 W PoE IEEE 802.bt
B.	Window Heater:	≤68° F (20° C) On; ≥86° F (30° C) Off (10 W)
C.	Fan:	≥95° F (35° C) On; ≤77° F (25° C) Off (2 W)
D.	Camera:	13.5 W
E.	IR LEDs	2 LEDs; 12 W; 164-459 ft (50-140 m) range; 
                                             beam angle selectable, 10-40; wavelength 850 nm
F.	Housing Connectors:	PoE Power Distribution Board: PoE in/Out; I/O terminal 
                                             block; IR connections/DIP switch
A.	Camera Connectors:	PoE Power: RJ-45; Video/Data: RJ-45; 
                                             Audio Input/Output: terminal block; audio level alarm 
                                             alert; Slot for SD card (supplied); Reset button; 
                                             Default button

2.05	CAMERA HOUSING ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-4° to 149°F (-20° to 65°C); 122° F (50° C) with IR LEDs

2.06	CAMERA KIT PHYSICAL SPECIFICATIONS

A.	Construction:	Cast aluminum 
B.	Viewing Window:	Chemically strengthened glass
C.	Cabling:	4x M16 waterproof cable glands
D.	Coating:	White epoxy powder
E.	External Dimensions:	H x L: 9.52 in. (241.7 mm) x 19.8 in. (502.8 mm)
F.	Usable Area Dimensions:	4.13 in. (105 mm) (W) x 3.05 in. (77.4 mm) (H) x 
                                             10.03 in. (255 mm) (L)
G.	Weight:	13 lb (5.9 kg)

2.07	LPR SPECIFICATION

A.	Region of Interest:		Provides calibration pattern for easy setup
B.	Lists: 			Standard allowlist/blocklist and custom lists; 50 user-
                                             defined lists including 4 pre-defined lists; list 
                                             synchronization between cameras on the system. 
                                             Schedules and rules management for each list.
                                            10,000 max plates per list.
C.	Event Responses: 		Vicon VMS Valerus, alarm out and FTP
D.	Event Logs: 		Search capabilities with captured image and plate 
                                              thumbnail
E.	Storage Options: 		Customizable
F.	Number of Events on 
SD Card: 			Up to 800,000 events on 32 GB card supplied 
                                             (25,000 events/GB)
G.	Recognition Rate: 		95%-99%, depending on country and installation 
                                             conditions
H.	Direction Detection: 	Yes
I.	Installation Parameters: 	Vehicle Speed: 15 mph (20 km/hr) max
                                             Detection Time: 100-1000 ms
                                             Character Height: Pixels:13 min; 25 recommended
                                             Target Distance: 16-100 ft (5-30.48 m)
                                             Maximum Horizontal/Vertical Angle: 35º max; 20º 
                                             recommended/35º max; 20º recommended
                                             Lane Coverage: Two max; 1 recommended
                                             Application: Vehicle entry/exit

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate: 8 MP: 3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240
Max 30 fps 
F.	Web Browser:	Safari, Firefox, Chrome, Microsoft Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             dynamic ROI
I.	Intelligent Video Analytics:	Tampering, Intelligent Motion Detection Intrusion 
                                             Detection, Line Cross, Loitering, Object 
                                             Left/Removed, Tailgating, Crowding; LPR; Museum 
                                             Search
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/Q/T

2.09	CERTIFICATIONS

A.	CE
B.	UL Listed
C.	FCC, Class A
D.	IP68 (Ingress Protection Rating)
E.	IK10 (Impact Rating including front glass)
F.	ONVIF: The product is conformant with Profiles S, T, G and Q and has been listed on the “Conformant Products” page of the onvi.org.
G.	RoHS (Restriction of Hazardous Substances in Electrical and Electronic Equipment) 
H.	NDAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The camera kit shall be Vicon Industries V2008-W0950-LPR and shall include an iCS lens and housing with wall mount bracket and IR illuminator module. An SD card and LPR license shall also be provided.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.