Vicon® Industries V2008B-LPR SERIES OUTDOOR IP BULLET CAMERA WITH LICENSE PLATE RECOGINITION (LPR)
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	IP BULLET CAMERA 

A.	The IP bullet camera shall incorporate a fixed camera/lens combination and embedded License Plate Recognition (LPR) technology; the license shall be included. The bullet camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall be available in 8 MP resolution model and shall have true WDR and Smart IR/Adaptive capability; includes an integral 
3.6-10 mm or 8-18 mm lens varifocal DC-iris lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 131 ft (40 m) with 4 IR LEDs. 

B.	The LPR software shall allow capture, storing and searching on an unlimited number of license plates and allow examination of details such as vehicle color, make and model. Customized lists of license plates shall be able to be created to generate an alert; lists shall be able to be synchronized from one camera to other cameras on the system. On-screen alarm handling procedures shall provide step-by-step instructions for addressing alarms. License plates from over 70 countries shall be supported. The ability to search by plate shall be available. Having the LPR analytic on the edge shall allow for a standalone LPR solution for users who do not want to integrate with a compatible VMS; it shall be able to integrate with the manufacturer’s video management system to monitor events through its Alarms Management suite. When the LPR camera is used with Valerus, the powerful alarm handling procedures shall give you step-by-step instructions for proactively addressing alarms and alerts. For example, you shall be able to create multiple customized lists of “allow” license plates that are associated with executives, VIPs, etc. These plates shall generate an alert upon entry, and stakeholders shall be immediately notified and provided with a list of to-dos, like unlock certain doors, turn on lights, etc. Similarly, license plates on the “block” list shall have unique procedures that you can easily follow for threat mitigation.

C.	The bullet camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and rotation (roll), for any angle of view required. A variety of mounting options shall be available. 

D.	The bullet camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross, loitering, object left/removed, tailgating and crowding. 

E.	The bullet camera shall be powered by PoE+, 24 VAC or 12 VDC. A dual heater system shall be provided; It maintains proper temperature in the camera housing and prevents fogging of the window. For low temperature operation: heater turns on at -40° F (-40° C) and off at 59° F (15° C). For defog operation: heater turns on at -40° F (-40° C) and off at 140° F (60° C.

F.	The bullet camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG image compression. The camera shall also have smart encoding to further improve video encoding and storage capacity.

G.	The bullet camera features shall include motorized autoiris, Automatic Gain Control (AGC), True Wide Dynamic Range (TWDR), white balance, defog, flip, mirror, privacy masking, Dynamic Region of Interest (ROI), Backlight Compensation (BLC) / Highlight Compensation (HLC) and motion detection.

H.	The bullet camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance, including front glass. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

I.	The bullet camera shall include a slot for an SD card for local storage. 32 GB SD card shall be provided. If other SD card is used its requirements are: Class 10; read speed: 100 MB/sec; write speed: 60 MB/sec.

J.	The bullet camera shall meet or exceed the following design and performance specifications.

2.03	IP BULLET CAMERA SPECIFICATIONS 

A.	Imaging Device:	1/1.8-inch progressive scan
B.	Max. Resolution:	3840 x 2160 (8 MP) 
C.	Shutter Speed:	Auto (1/2 - 1/10,000 sec), manual
D.	Automatic Gain Control:	On/Off selectable
E.	Minimum Illumination	Color: 3.6-10 mm: 0.02 lux or 8-18 mm: 0.01 lux; B&W: 0.01 lux/0 lux (IR Off/On)
F.	Tilt and Horizontal	Three-direction adjustment, allowing for adjustment of 
                                              pan, tilt and rotation (roll)
G.	Digital Zoom:	Yes (DROI)
H.	Lens Adjustment:	Motorized lens, P-iris automatically adjusts to zoom 
                                              condition
I.	Focal Length:	3.6-10 mm; 2.8X optical zoom or 8-18 mm; 2.5X
J.	Horizontal Field of View:	3.6-10 mm: 98°-46° (wide-tele) or 
                                             8-18 mm:  60°-256° (wide-tele)
K.	Vertical Field of View:	3.6-10 mm: 54°-26° (wide-tele) or 
                                              8-18 mm:  33°-12° (wide-tele)
L.	IR Distance:	Smart IR/Adaptive IR; 131 ft (40 m) with 4 IR LEDs
M.	Dual Heater System:	For low temperature operation: heater turns on at -40° F 
                                             (-40° C) and off at 59° F (15° C). 
                                             For defog operation: heater turns on at -40° F and off at
                                             140° F (60° C).
2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	24 VAC, 12 VDC or PoE+
B.	Current:	PoE: 0.41 A; 24 VAC: 0.82 A; 12 VDC: 1.64 A 
C.	Power Consumption:	IR/Heaters On: IR/Heaters On: 19.68 W; 
                                              IR Off/Heaters On: 12.48 W
D.	Connectors:	Pigtail cable provided; optional backbox required for
                                             cabling
                                             Power: 12 VDC or 24 VAC terminal block
	PoE: RJ-45
		Video/Data: RJ-45
		Alarm: screw terminal
		Audio: screw terminal; audio level alarm alert
		Slot for SD card (supplied)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 140°F (-40° to 60°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum alloy body; sunshield: PC+ABS
B.	Dimensions:	Length: 10.3 in. (261 mm), 
Diameter: 3.5 in. (89 mm)
C.	Weight: 	4 lb (1.8 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3-axis camera adjustment: pan 360°; tilt 0°-90°; 
roll 360° 

2.08	LPR SPECIFICATION

A.	Region of Interest:		Provides calibration pattern for easy setup
B.	Lists: 			Standard allowlist/blocklist and custom lists; 50 user-
                                             defined lists including 4 pre-defined lists; list 
                                             synchronization between cameras on the system. 
                                             Schedules and rules management for each list.
                                            10,000 max plates per list.
C.	Event Responses: 		Vicon VMS Valerus, alarm out and FTP
D.	Event Logs: 		Search capabilities with captured image and plate 
                                              thumbnail
E.	Storage Options: 		Customizable
F.	Number of Events on 
SD Card: 			Up to 800,000 events on 32 GB card supplied 
                                             (25,000 events/GB)
G.	Recognition Rate: 		95%-99%, depending on country and installation 
                                             conditions
H.	Direction Detection: 	Yes
I.	Installation Parameters: 	Vehicle Speed: 15 mph (20 km/hr) max
                                             Detection Time: 100-1000 ma
                                             Character Height: Pixels:13 min; 25 recommended
                                             Target Distance: 6.6-19.7 ft (2-6 m)
                                             Maximum Horizontal/Vertical Angle: 35º max; 20º 
                                             recommended/35º max; 20º recommended
                                             Lane Coverage: Two max; 1 recommended
                                             Application: Vehicle entry/exit

2.09	  NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	2 MP: 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240 
5 MP: 2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180
8 MP: 3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:	Tampering/Defocus, Intelligent Motion Detection 
                                             Intrusion Detection; Line Cross, Loitering, 
                                             Object Left/Removed, Tailgating, Crowding
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/Q/T

2.10	CERTIFICATIONS

A.	CE
B.	UL Listed
C.	FCC, Class A
D.	IP67 (Ingress Protection Rating)
E.	IK10 (Impact Rating including front glass)
F.	ONVIF: The product shall be conformant with Profiles S, T, G and Q and has been listed on the “‘Conformant Products” page of the onvi.org.
G.	RoHS (Restriction of Hazardous Substances in Electrical and Electronic Equipment) 
H.	NDAA/GSA/TAA compliant

2.11	WARRANTY

A.	5 years, parts and labor

2.12	APPROVED MANUFACTURERS

A.	The outdoor IP bullet camera shall be Vicon Industries V2008B-W310LPR and V2008B-W818LPR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.