Vicon® Industries V2100B OUTDOOR IP BULLET CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP BULLET CAMERA 

A.	The outdoor bullet camera shall incorporate a fixed camera/lens combination. The bullet camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera be available in a 5 MP resolution model and shall have true WDR and Smart IR capability and include a 3.1-10 mm lens integral varifocal DC-iris lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft (30 m) with 16 IR LEDs. 

B.	The camera position shall have a two-direction adjustment, allowing for adjustment of pan and tilt, for any angle of view required. A variety of mounting options shall be available. 

C.	The bullet camera shall be powered by PoE or 12 VDC. 

D.	The bullet camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

E.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection. It shall have Video Content Analysis (VCA) of motion and tampering/defocus.

F.	The bullet camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK08 rated for impact resistance. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

G.	The bullet camera shall provide a slot for an SD card for local storage.

H.	The bullet camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP BULLET CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.8-inch progressive scan 
B.	Max. Resolution:	5 MP model
C.	Shutter Speed:	1/2 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity (@30 IRE):	5 MP: Color: 0.05 lux; B&W: 0.03 lux/0 lux (IR Off/On)
F.	Tilt and Horizontal	Two-direction adjustment, allowing for adjustment of 
                                              pan and tilt
G.	Digital Zoom:	Yes (ROI)
H.	Lens Adjustment:	Motorized lens, DC-iris 
I.	Focal Length:	3.1-10 mm varifocal 
J.	Horizontal Field of View:	96°-32° (wide-tele)
K.	Vertical Field of View:	69°-24° (wide-tele)
L.	Depth Field of View:	124°-40° (wide-tele)
M.	IR Distance:	Smart IR; 98 ft (30 m) with 16 IR LEDs

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC or PoE
B.	Current:	PoE: 0.16 A; 12 VDC: 0.63 A 
C.	Power Consumption:	IR On: 7.6 W; IR Off: 5.2 W 
D.	Connectors:	Pigtail cable provided; optional backbox required for
                                             cabling
                                             Power: 12 VDC terminal block
	PoE: RJ-45
		Video/Data: RJ-45
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-22° to 140°F (-30° to 60°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum alloy body; bracket: PC+ABS; 
                                             window: double glass/polycarbonate
B.	Dimensions:	Length: 6.9 in. (177 mm), 
Width: 3.3 in. (84 mm)
Height: 3.1 in. (79 mm)
C.	Weight: 	2 lb (0.9 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	2-axis camera adjustment: pan 360°; tilt 0°-90° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	5 MP: 2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Video Content Analysis 
(VCA):	Tampering/defocus, motion
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP67
E.	IK08
F.	ONVIF S/T/G
G.	RoHS
H.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP bullet camera shall be Vicon Industries V2105B-W313MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.