Vicon® Industries V810B SERIES OUTDOOR IP BULLET CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP BULLET CAMERA 

A.	The outdoor bullet camera shall incorporate a camera/lens combination. The dome camera shall be available for surface mounting on an integral wall mount. The high-resolution day/night camera shall have WDR and IR capability and include an integral fixed or motorized varifocal autoiris lens. Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft (30 m). 

B.	The camera position shall allow for adjustment of angle of view on its integral wall mount. 

C.	The camera shall have smart encoding, which monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.

D.	The camera shall be powered by PoE or 12 VDC. 

E.	The camera shall have triple streaming video and support H.264/H.265, and 
M-JPEG compression. The camera shall be available in 1080p (2 MP) and 4 MP resolution. 

F.	Camera features shall include electronic iris, WDR, digital zoom, white balance, flip and mirror, privacy masks, museum search and motion detection.

G.	The camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface.

H.	The camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP CAMERA DOME SPECIFICATIONS

A.	Imaging Device:	2 MP: 1/2.9-inch progressive scan CMOS; 
	4 MP: 1/3-inch progressive scan CMOS;
B.	Max. Resolution:	1080p (2 MP) and 4 MP models
C.	Shutter Speed:	1 - 1/10,000 sec
D.	Digital Zoom:	Yes
E.	Sensitivity:	Color: 0.1 lux; B&W: 0 lux (IR On) @f/2.1
F.	Tilt and Horizontal	Adjust camera position on integral wall mount. 
Adjustment:	Mechanical adjustment: pan (360°), tilt (90°) and	
	roll (360°)
G.	Lens Adjustment:	Fixed or motorized focus and zoom adjustment 
H.	Focal Length:	Fixed models: 3.6 mm 
	Motorized models: 2.8-12 mm varifocal
I.	Horizontal Field of View:	Fixed models: 84° 
	Motorized models: 95°- 35°
J.	IR Distance:	98 ft (30 m 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE, 12 VDC 
B.	Current (IR on):	PoE: 87 mA/106 mA (fixed); 280 mA (motorized)
                                             12 VDC: 145 mA (fixed); 520 mA/480 mA (motorized)
C.	Power Consumption 
(IR on):	PoE: 4.2 W/5.1 W (fixed); 7 W (motorized)
	12 VDC: 3.4 W/3.8 W (fixed); 6.2 W/5.8 W (motorized)
D.	Connectors:	Power: standard jack for adapter 
	PoE/Network: RJ-45
		
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	14° to 122°F (-10° to 50°C) 

B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum
B.	Dimensions:	Fixed series: Length: 6.1 in. (155 mm), 
Diameter: 3.0 in. (77 mm)
Motorized Series: Length: 9.4 in. (239 mm), 
Diameter: 3.3 in. (84 mm)
C.	Weight: 	Fixed: 0.66 lb (0.3 kg); Motorized: 1.5 lb (0.68 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Integral wall mount for surface mounting 
B.	Adjustments:	Mechanical adjustment, pan (360°), tilt (90°) and roll/azimuth (360°) 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management Systems 
B.	Compression:	H.264/H.265; M-JPEG available 
C.	LAN Interface:	10 Base-T/100 Base-TX
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	1080p (2 MP): 1920x1080, 1440x1080, 
				1280x1024,1280x720/960, 720P), 1024x768, 
				704x480/576 (D1), 640x480 (VGA), 400x240, 
				320x240 (QVGA)
				4 MP: 2592x1520, 2304x1296, 1920x1080 (1080P), 
				1440x1080, 1280x1024, 1280x720/960 (720P), 
				1024x768, 704x480/576 (D1), 640x480 (VGA), 400x240, 
				320x240 (QVGA
Max 30 fps at 1920x1080; 20 fps @ 4 MP
F.	Web Browser:	Internet Explorer, Chrome, Safari, Firefox 
G.	Users:	Up to 10 clients
H.	Image Settings:	Day/night mode; flip and mirror; configurable 
                                             brightness, contrast, chroma, sharpness, saturation; 
	white balance; Electronic Shutter, automatic or manual;
                                             true WDR; privacy masks (4); motion detection (16); 
	DNR; digital zoom
I.	Video Content Analytics:	Defog, Intrusion Detection, Intelligent Video Motion 
	Detection, Museum Search and Camera Tampering
J.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             DHCP, FTP, UDP, uPnP,QoS, Zeroconfig, Bonjour

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The indoor fixed color IP dome camera shall be Vicon Industries Model V812D-WIR, V812D-W312MIR, V814D-WIR and V814D-W312MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.