Vicon® Industries V930D SERIES OUTDOOR IP TURRET CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP TURRET CAMERA 

A.	The outdoor turret camera shall incorporate a camera/lens combination. The camera shall be available for outdoor surface mounting. The high-resolution day/night camera shall have WDR and IR capability and include an integral fixed lens. Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft 
(30 m) with 15 IR LEDs. 

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation (roll), for any angle of view required.

C.	The camera shall have smart encoding, which monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.

D.	The camera shall be powered by PoE or 12 VDC. 

E.	The camera shall have triple streaming video and support H.264/H.265, and 
M-JPEG compression. The camera shall be available in 1080p (2 MP) and 4 MP resolution. 

F.	Camera features shall include electronic iris, WDR, digital zoom, white balance, flip and mirror, museum search, privacy masks and motion detection.

G.	The camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface.

H.	The camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP TURRET CAMERA SPECIFICATIONS

A.	Imaging Device:	2 MP: 1/2.9-inch progressive scan CMOS; 
	4 MP: 1/3-inch progressive scan CMOS
B.	Max. Resolution:	1080p (2 MP) and 4 MP models
C.	Shutter Speed:	1 - 1/10,000 sec
D.	Digital Zoom:	Yes
E.	Sensitivity:	Color: 0.1 lux; B&W: 0 lux (IR On) @f/2.1
F.	Tilt and Horizontal	3-axis adjustment: pan, tilt and roll (lens	may be rotated Adjustment:	on its axis); camera mechanical tilt angle of 70°
G.	Lens Adjustment:	Fixed 
H.	Focal Length:	3.6 mm 
I.	Horizontal Field of View:	84° 
J.	IR Distance:	98 ft (30 m); 15 IR LEDs 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE, 12 VDC 
B.	Current (IR on):	PoE: 106 mA/124 mA 
                                             12 VDC: 360 mA/380 mA)
C.	Power Consumption 
(IR on):	PoE: 5.1 W/6 W; 12 VDC: 4.3 W/4.6 W
D.	Connectors:	Power: standard jack for adapter 
	PoE/Network: RJ-45
		
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	14° to 122°F (-10° to 50°C) 

B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum
B.	Dimensions:	Height: 3.4 in. (85.1 mm), 
Diameter: 3.5 in. (90.1 mm)
C.	Weight: 	0.55 lb (0.250 kg

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3 axis adjustment, pan, tilt and roll/azimuth; camera mechanical tilt angle of 70°

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management Systems 
B.	Compression:	H.264/H.265; M-JPEG available 
C.	LAN Interface:	10 Base-T/100 Base-TX
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	1080p (2 MP): 1920x1080, 1440x1080, 
				1280x1024,1280x720/960 (720P), 1024x768, 
				704x480/576 (D1), 640x480 (VGA), 400x240, 
				320x240 (QVGA)
				4 MP: 2592x1520, 2304x1296, 1920x1080 (1080P), 
				1440x1080, 1280x1024, 1280x720/960 (720P), 
				1024x768, 704x480/576 (D1), 640x480 (VGA), 400x240, 
				320x240 (QVGA)
Max 30 fps at 1920x1080
F.	Web Browser:	Internet Explorer, Chrome, Safari, Firefox 
G.	Users:	Up to 10 clients
H.	Image Settings:	Day/night mode; flip and mirror; configurable 
                                             brightness, contrast, chroma, sharpness, saturation; 
	white balance; Electronic Shutter, automatic or manual;
                                             WDR; privacy masks (4); motion detection (16); 
	DNR; digital zoom
I.	Video Content Analytics:	Intrusion Detection, Museum Search, Intelligent Video 	Motion Detection and Tampering
J.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             DHCP, FTP, UDP, uPnP,QoS, Zeroconfig, Bonjour

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP turret camera shall be Vicon Industries Model V932D-IR-1 and V934D-IR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.