Vicon® Industries V9360-6 AND V9360-12 SERIES HEMISPHERIC DOME CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	HEMISPHERIC IP CAMERA DOME

A.	The hemispheric dome cameras shall be available in indoor and outdoor models, each in 6 MP or 12MP. It shall incorporate a fixed camera/lens combination. The camera dome shall be available for surface mounting; other mounting options shall be available. The high-resolution day/night camera shall have WDR and IR capability and be include an integral 1/1.8 or 1/1.7 inch fisheye lens (6 MP/12 MP). This lens shall provide an extremely wide angle of view for a panoramic image, capturing a complete 360° view at full HD resolution. Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 16 ft (5 m). 

B.	The camera shall provide a high-resolution hemispherical view and shall provide crisp distortion free images. Edge dewarping shall be done within the camera itself; software dewarping shall be available for those VMS systems that support it. Multiple dewarp display modes shall be available.

C.	The dome camera shall be powered by PoE or 12 VDC. 

D.	The dome camera shall provide dual streams video based on two configuration in single view mode; multiple streams based on single configuration in 6 cropped VGA mode shall also be available. The camera shall support H.264 and M-JPEG compression.

E.	Camera features shall include electronic iris.

F.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface. All models shall have an IK10 rating; the outdoor models shall be IP66-rated to withstand rain, dust and vandalism.

G.	The dome camera shall provide a slot for an SD card for local storage.

H.	Two-way audio shall be provided; the indoor model shall have built in speaker and microphone.

I.	The hemispheric dome camera shall meet or exceed the following design and performance specifications.

2.03	
DAY/NIGHT IP CAMERA DOME SPECIFICATIONS

A.	Imaging Device:	6 MP: 1/1.8-inch progressive scan CMOS 
                                             12 MP: 1/1.7-inch progressive scan CMOS
B.	Max. Resolution:	6 MP or 12 MP models
C.	Shutter Speed:	1 - 1/10,000 sec
D.	Automatic Gain Control:	On (1-3)/Off selectable
E.	Sensitivity:	6 MP: Color: 0.04 lux; B&W: 0.002 lux;
12 MP: Color: 0.1 lux; B&W: 0.01 lux
F.	Digital Zoom:	Yes 
G.	Lens Adjustment:	Fisheye lens: 
                                              6 MP: 1/2”, F1.6; M12 mount
                                             12 MP: 1/1.7”, F2.8; M12 mount
H.	Focal Length:	6 MP: 1.6 mm 
                                             12 MP: 1.65 mm
I.	Angle of View:	6 MP: 185° at full resolution 
                                             12 MP: 190° at full resolution
J.	IR Distance/Sensitivity:	16 ft (5m)/850 nm; 4 LEDs 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC or PoE
B.	Current (IR on):	PoE: 0.14 A; 
                                             12 VDC: 0.675 A; 
C.	Power Consumption:	PoE: 7.1 W; 
                                             12 VDC: 8.1 W; IR On: +1.9 W
D.	Connectors:	Power: 12 VDC screw terminal or PoE RJ-45
	Network (Video/Data): RJ-45
		Alarm In/Out: screw terminal
		Audio In/Out: screw terminal (indoor); phone jack with cable (outdoor)
		Slot for SDXC card
		Default
		Outdoor model provides pigtail connection
E.	Radio Frequency	Default button
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	Indoor: 14° to 122°F (-10° to 50°C) 
                                             Outdoor: -22° to 122°F (-30° to 50°C)

B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum

B.	Dimensions:	Height: 2.17 in. (55 mm), 
Diameter: 4.6 in. (117 mm) 
C.	Weight: 	0.88 lb (0.40 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount (2 mounting holes); mounting options available 
2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management System 
B.	Compression:	H.264; M-JPEG 
C.	LAN Interface:	1 Gbps Ethernet
D.	Video Channels	Quad streaming
E.	Resolution and Frame Rate:	3072x2048 (6 MP)/4000x3000 (12 MP) max. 
Max 60 fps depending of video streaming and dewarping type.
F.	Web Browser:	Internet Explorer 7.0 and above, Safari, Firefox
G.	Users:	Up to 20 clients
H.	Image Settings:	Configurable brightness, contrast, hue, sharpness. 
	saturation; white balance; WDR; exposure; edge 
	dewarping; DNR (3D); privacy masks; ICR; Smart 
                                              Events (tampering alarm, motion detection, network 
                                              failure, audio detection, manual tripper event, periodic 
                                              event), IR threshold, BLC; digital zoom, ROI, text 
                                              overlay    
I.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTP 
                                             SMTP, DHCP, PPPoE, IGMP, FTP, ICMP, UDP, 
	uPnP, QoS, SNMP, ARP, ONVIF 

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP66 (outdoor models)
E.	IK10
F.	RoHS

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor hemispheric IP dome cameras shall be Vicon Industries Model 
V9360W-6 and V9360W-12; the indoor models shall be Model V9360-6 and 
V9360-12.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.