Vicon® Industries V940B SERIES OUTDOOR IP BULLET CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP BULLET CAMERA 

A.	The outdoor fixed bullet camera shall incorporate a camera/lens combination. The camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall have true WDR and IR capability and include an integral varifocal autoiris lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft (30 m) with smart IR LED technology. 

B.	The camera position shall be adjustable using the integral mount. A sunshield shall be provided.

C.	The camera shall have smart encoding, which monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.

D.	The camera shall be powered by PoE, 24 VAC or 12 VDC. 

E.	The camera shall have triple streaming video and support H.264/H.265, and 
M-JPEG (3rd stream only) compression. The camera shall be available in 1080p
(2 megapixel), 4 MP and 5 MP resolution. There shall be additional 2 MP models available with ultra-high-sensitivity and extended WDR (132 dB).

F.	Camera features shall include electronic iris, AGC, WDR, white balance, corridor, mirror, privacy masks, ROI (Region of Interest), museum search and motion detection.

G.	The camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance.

H.	The camera shall provide a slot for an SD card for local storage.

I.	There shall be a back box for ease of cabling.

J.	The camera shall meet or exceed the following design and performance specifications.
2.03	DAY/NIGHT IP BULLET CAMERA SPECIFICATIONS

A.	Imaging Device:	2/4 MP: 1/3-inch progressive scan CMOS; 
	2 MP-XW: 1/2.8-inch progressive scan CMOS; 
	2 MP-XS: 1/1.9-inch progressive scan CMOS; 
	5 MP: 1/1.8-inch progressive scan CMOS;
B.	Max. Resolution:	1080p (2 MP), 4 MP and 5 MP models
C.	Shutter Speed:	2 MP/4 MP: 1 - 1/32,000 sec
	2 MP-XW/2 MP-XS/5 MP: 1 - 1/30,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity:	2 MP/2 MP-X/4 MP: Color: 0.01 lux; B&W: 0 lux (IR On)
@f/1.4, 30 IRE, AGC On
2 MP-XS: Color: 0.002 lux; 
B&W: 0.0006 lux/0 lux (IR On) @f/1.5, AGC On
5 MP: Color: 0.1 lux; B&W: 0.02 lux/0 lux (IR On)
@f/1.5, AGC On
F.	Wide Dynamic Range	True WDR, 120dB; XW: 132dB
G.	Tilt and Horizontal	3-axis adjustment: pan (360°), tilt (80°) and roll (lens Adjustment:	may be rotated on its axis 360°)
H.	Lens Adjustment:	Motorized focus and zoom adjustment 
I.	Focal Length:	2 MP/4 MP: 2.7-12 mm varifocal 
	2 MP-XW: 3-10.5 mm varifocal
	2 MP-XS/5 MP: 3.6-10 mm varifocal
J.	Horizontal Field of View:	2 MP: 85°- 29.8°
	2 MP-XW: 92.5°- 33°
	2 MP-XS: 101.8°- 44.3°
	4 MP: 94°- 31°
	5 MP: 87.9°- 38.4°
K.	IR Distance:	98 ft (30 m) 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE, 24 VAC, 12 VDC 
B.	Current (IR on):	24 VAC: 427 mA; 
                                             12 VDC: 833 mA; 
C.	Power Consumption 
(IR on):	<10 W; 
D.	Connectors:	Power: standard jack for adapter 
	PoE/Network: RJ-45
		Alarm: screw terminal
		Audio: RCA jack
		Slot for SD card
		BNC Composite output for installation
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 140°F (-40° to 60°C) 

B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum
B.	Dimensions:	Height: 3.33 in. (84.6 mm), 
Width: 3.54 in. (90 mm),
Depth: 11.83 in. (300.4 mm)
C.	Weight: 	Approximately 2.09 lb (0.95 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Integral wall mount 
B.	Adjustments:	Tilt adjustment 90° and rotation of 360° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management Systems 
B.	Compression:	H.264/H.265; M-JPEG available 
C.	LAN Interface:	10 Base-T/100 Base-TX
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	1080p (2 MP) Major streams: 1920x1080, 1280x720/960
				4 MP Major streams: 2592x1520, 2048x1520, 
				2304x1296,1920x1080, 1280x720/960
				5 MP: Major streams: 2592x1944, 2592x1520, 
				2048x1520, 2304x1296,1920x1080, 1280x720/960
Max 30 fps at 1920x1080
F.	Web Browser:	Internet Explorer (min IE8)
G.	Users:	Up to 10 clients
H.	Image Settings:	Day/night mode; corridor and mirror; configurable 
                                             brightness, contrast, hue, sharpness, saturation; white 
                                             balance, AGC; Electronic Shutter, automatic or manual;
                                             true WDR (120dB or 132dB on XW model); privacy 
	masks (4); motion detection (4); 	ROI (8); DNR
I.	Video Content Analytics:	EIS, Defog, Video Contents Analysis (Intrusion 
	Detection, Line Cross Detection, Museum Search and 	Camera Tampering – Scene Change, Defocus, 
	Low/High Brightness)
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             SMTP, DHCP, NTP, FTP DDNS, UDP, uPnP,QoS, 
                                             ARP, IGMP, SNMP (V3), TLS, SSL, 802.1x, PPPoE, 
				DNS, ICMP

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	IP67
D.	IK10

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor fixed color IP bullet camera shall be Vicon Industries Model V942B-W312MIR, V942B-W312MIR-XW, V942B-W312MIR-XS, V944B-W312MIR, and V945B-W310MIR.
END OF SECTION
Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.