Vicon® Industries V940D SERIES OUTDOOR FIXED IP DOME CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR FIXED IP DOME CAMERA 

A.	The outdoor fixed dome camera shall incorporate a camera/lens combination. The dome camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall have true WDR and IR capability and include an integral varifocal autoiris lens. The lens shall be motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft (30 m) with smart IR LED technology. A clear polycarbonate lower dome that is secured by tamperproof screws shall be included. 

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation (roll), for any angle of view required.

C.	The dome camera shall have smart encoding, which monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.

D.	The dome camera shall be powered by PoE, 24 VAC or 12 VDC. 

E.	The dome camera shall have triple streaming video and support H.264/H.265, and 
M-JPEG (3rd stream only) compression. The camera shall be available in 1080p
(2 megapixel), 4 MP and 5 MP resolution. There shall be additional 2 MP models available with ultra-high-sensitivity and extended WDR (132 dB).

F.	Camera features shall include electronic iris, AGC, WDR, white balance, corridor, mirror, privacy masks, ROI (Region of Interest), museum search and motion detection.

G.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface. It shall be IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance.

H.	The dome camera shall provide a slot for an SD card for local storage.

I.	There shall be mounting accessories to allow pendant mounting, mounting to a 4x4 electrical box and a back box for ease of cabling.

J.	The fixed-position camera dome shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP CAMERA DOME SPECIFICATIONS

A.	Imaging Device:	2/4 MP: 1/3-inch progressive scan CMOS; 
	2 MP-XW: 1/2.8-inch progressive scan CMOS; 
	2 MP-XS: 1/1.9-inch progressive scan CMOS; 
	5 MP: 1/1.8-inch progressive scan CMOS;
B.	Max. Resolution:	1080p (2 MP), 4 MP and 5 MP models
C.	Shutter Speed:	2 MP/4 MP: 1 - 1/32,000 sec
	2 MP-XW/2 MP-XS/5 MP: 1 - 1/30,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity:	2 MP/2 MP-X/4 MP: Color: 0.01 lux; B&W: 0 lux (IR On)
@f/1.4, 30 IRE, AGC On
2 MP-XS: Color: 0.002 lux; 
B&W: 0.0006 lux/0 lux (IR On) @f/1.5, AGC On
5 MP: Color: 0.1 lux; B&W: 0.02 lux/0 lux (IR On)
@f/1.5, AGC On
F.	Wide Dynamic Range	True WDR, 120dB; XW: 132dB
G.	Tilt and Horizontal	3-axis adjustment: pan (360°), tilt (80°) and roll (lens Adjustment:	may be rotated on its axis 360°)
H.	Lens Adjustment:	Motorized focus and zoom adjustment 
I.	Focal Length:	2 MP/4 MP: 2.7-12 mm varifocal 
	2 MP-XW: 3-10.5 mm varifocal
	2 MP-XS/5 MP: 3.6-10 mm varifocal
J.	Horizontal Field of View:	2 MP: 85°- 29.8°
	2 MP-XW: 92.5°- 33°
	2 MP-XS: 101.8°- 44.3°
	4 MP: 94°- 31°
	5 MP: 87.9°- 38.4°
K.	IR Distance:	98 ft (30 m) 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE, 24 VAC, 12 VDC 
B.	Current (IR on):	24 VAC: 375 mA; 
                                             12 VDC: 750 mA; 
C.	Power Consumption 
(IR on):	<9 W; 
D.	Connectors:	Power: standard jack for adapter 
	PoE/Network: RJ-45
		Alarm: screw terminal
		Audio: RCA jack
		Slot for SD card
		BNC Composite output for installation
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 140°F (-40° to 60°C) 

B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum
Dome: clear polycarbonate; tamperproof screws
B.	Dimensions:	Height: 4.76 in. (121 mm), 
Diameter: 5.91 in. (150 mm)
C.	Weight: 	Approximately 2.32 lb (1.05 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3 axis adjustment, pan (360°), tilt (80°) and roll/azimuth (360°) 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management Systems 
B.	Compression:	H.264/H.265; M-JPEG available 
C.	LAN Interface:	10 Base-T/100 Base-TX
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	1080p (2 MP) Major streams: 1920x1080, 1280x720/960
				4 MP Major streams: 2592x1520, 2048x1520, 
				2304x1296,1920x1080, 1280x720/960
				5 MP: Major streams: 2592x1944, 2592x1520, 
				2048x1520, 2304x1296,1920x1080, 1280x720/960
Max 30 fps at 1920x1080
F.	Web Browser:	Internet Explorer (min IE8)
G.	Users:	Up to 10 clients
H.	Image Settings:	Day/night mode; corridor and mirror; configurable 
                                             brightness, contrast, hue, sharpness, saturation; white 
                                             balance, AGC; Electronic Shutter, automatic or manual;
                                             true WDR (120dB or 132dB on XW model); privacy 
	masks (4); motion detection (4); 	ROI (8); DNR
I.	Video Content Analytics:	EIS, Defog, Video Contents Analysis (Intrusion 
	Detection, Line Cross Detection, Museum Search and 	Camera Tampering – Scene Change, Defocus, 
	Low/High Brightness)
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             SMTP, DHCP, NTP, FTP DDNS, UDP, uPnP,QoS, 
                                             ARP, IGMP, SNMP (V3), TLS, SSL, 802.1x, PPPoE, 
				DNS, ICMP

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	IP66
D.	IK10

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor fixed color IP dome camera shall be Vicon Industries Model V942D-W312MIR, V942D-W312MIR-XW, V942D-W312MIR-XS, V944D-W312MIR, and V945D-W310MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.