Vicon® Industries V988D OUTDOOR IP 4K DOME CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP BULLET CAMERA 

A.	The outdoor fixed dome camera shall incorporate a fixed camera/lens combination. The camera dome shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall have true WDR and IR capability and include an integral 3.6-11 mm varifocal autoiris lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 90 ft (30 m) with 28 IR LEDs. 

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation (roll), for any angle of view required.

C.	The dome camera shall be powered by PoE or 12 VDC. A heater shall be provided. 

D.	The dome camera shall have quad streaming video and support H.264/H.265and 
M-JPEG compression. The camera shall have 4K (8 megapixel) resolution.

E.	Camera features shall include electronic iris, AGC, WDR, white balance, flip, mirror, privacy masking, ROI and motion detection.

F.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface. It shall be IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance.

G.	The dome camera shall provide a slot for an SD card for local storage.

H.	The dome camera shall meet or exceed the following design and performance specifications.

2.03	
DAY/NIGHT IP BULLET CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.5-inch progressive scan 
B.	Max. Resolution:	4K (8 MP)
C.	Shutter Speed:	1 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity:	Color: 0.03 lux; B&W: 0 lux (IR On);@f/1.6
F.	Tilt and Horizontal	Integral mount allows positioning adjustment
G.	Digital Zoom:	Yes (ROI)
H.	Lens Adjustment:	Motorized lens, iris automatically adjusts to zoom 
                                              condition
I.	Focal Length:	3.6-11 mm varifocal 
J.	Horizontal Field of View:	87°-38° 
K.	IR Distance:	90 ft (30m) with 28 IR LEDs

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC or PoE
B.	Current (IR on):	PoE: 200 mA; 
                                             12 VDC: 690 mA 
C.	Power Consumption 
(IR on):	PoE: 9.6 W; 
                                             12 VDC: 8.3 W
D.	Connectors:	Power: 12 VDC standard jack or 
	PoE RJ-45
		Video/Data: RJ-45
		Alarm: screw terminal
		Audio: screw terminal
		Slot for uSD card
		Composite output for installation
		Reset button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-4° to 131°F (-20° to 55°C) 
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum base; polycarbonate clear dome; 
                                             tamperproof screws
B.	Dimensions:	Height: 3.9 in. (99 mm), 
Diameter: 5.7 in. (144 mm)
C.	Weight: 	Approximately 1.7 lb (0.79 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3-axix camera adjustment: pan 360°; tilt 90°; roll 360° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus and ViconNet 
	Video Management System 
B.	Compression:	H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Quad streaming
E.	Resolution and Frame Rate:	3840x2160, 3072x2048, 2592x1944/1520, 2560x1440, 1920x1080, 1440x1080, 1280x1024/720, 1024x768, 800x600/480, 720x576/480, 704x480/576, 640x480, 352x240/288/256, 320x240;
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome
G.	Users:	Live viewing for up to 10 clients; playback 3 clients
H.	Image Settings:	Adjustable bit rate; flip and mirror; configurable 
                                             brightness, contrast, saturation, chroma, sharpness; 
	white balance, AGC; Electronic Shutter; automatic or 
	manual; digital zoom; motion detection; 
                                             zoom and focus (motorized lens models)
I.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS RTSP, RTCP, RTP 
                                             DHCP, FTP DDNS, UDP, QoS, ARP, Bonjour, Zeroconf, 

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	IP66
D.	IK10

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP dome camera shall be Vicon Industries Model V988D-W311MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.