Vicon® Industries V2008PTZ-IR NETWORK OUTDOOR PTZ DOME 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	NETWORK CAMERA DOME FEATURES

A.	The compact network dome shall be comprised of a camera/lens and pan/tilt drive in an attractive covert enclosure. It shall have 8 MP resolution and shall have true WDR. It shall include an integral varifocal 6.5-230 mm lens (35X optical zoom); it shall also have 8X digital zoom. Day/night operation shall be achieved using a built-in IR-cut filter. It shall have starlight low-light imaging. IR distance shall be 1312 ft (400 m) and it shall have Adaptive IR capability. 

B.	The dome camera shall provide Intelligent Video Analysis for tampering, motion detection and auto-tracking (people); it shall also support Museum Search.

C.	The dome camera shall have a speed-dry feature that shall remove water droplets from the exterior of the dome.

D.	The dome camera shall be powered by PoE++ or 24 VAC.

E.	The dome camera shall have triple streaming video and provide network video transmission using either H.264/H.265 and M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity. The camera dome shall transmit high quality video across the network for remote viewing and recording and shall be configurable remotely from network digital video recorders and master workstations.

A.	One alarm input shall be programmable for functional state (enabled or disabled); it shall be able to be set for Normally Open (NO) or Normally Closed (NC). The alarm output shall be able to control external equipment; it shall be able to be set for Normally Open (NO) or Normally Closed (NC). It shall have two-way audio capability (line in/line out).

B.	There shall be 256 individual programmable preset positions available. Each preset shall be able to have an individual title and shall be adjustable, lock or auto focus.

E.	There shall be eight tours available with up to 32 presets per tour. Each tour shall be able to have an individual title and shall be adjustable for pan, tilt and zoom speed and dwell time. Tours shall repeat by default.

F.	Pan and tilt functions shall be programmable. Maximum manual pan and tilt speeds shall be programmable. Maximum pan speed shall be 720 degrees/sec and maximum tilt speed shall be 540 degrees/sec. Pan and tilt speeds shall also be scalable to the zoom setting. The pan range shall be 360 degree continuous and tilt range shall be -20 to 90 degrees.

F.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, speed dry, optical image/lens stabilization (OIS) and motion detection.

G.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/M interface. It shall be IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance of the housing. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

H.	The dome camera shall provide a slot for an SD card for local storage.

I.	The dome camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP DOME CAMERA SPECIFICATIONS

A.	Imaging Device:	1/1.8-inch Sony Starvis Gen2 
B.	Max. Resolution:	8 MP 
C.	Shutter Speed:	1/7 - 1/16,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	WDR:	True WDR (130 dB)
F.	Sensitivity (@ 30 IRE):	Starlight; Color: 0.04 lux; B&W: 0.01 lux (IR Off; 0 lux IR On)
G.	Pan/Tilt Range:	360° continuous pan; -20° to 90° tilt
H.	Lens:	6.5 – 230 mm, 35X optical zoom
I.	Digital Zoom:	8X
J.	Lens Adjustment:	Motorized zoom and focus (autofocus), P-iris 
                                              automatically adjusts to zoom condition (manual mode)
K.	Horizontal Field of View:	60.4°-2.0° (wide-tele)
L.	Vertical Field of View:	35.9°-1.2° (wide-tele)
M.	IR Distance:	1312 ft (400 m); Adaptive IR 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	24 VAC (+20%/-10%) or PoE++ 
                                             (IEEE 802.3bt, Class 8) 
B.	Current:	24 VAC: 3.25 A; 
C.	Power Consumption:	Total 71 W.  
D.	Connectors:	Power: 24 VAC terminal block; PoE: RJ-45
	Video/Data: RJ-45
		Alarm: terminal block
		Audio: terminal block
		Slot for SD card (1 TB max customer-supplied)
		Reset button
		Network status LED
	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 149°F (-40° to 65°C);
                                             -40° to 158°F (-40° to 70°C) IR off for 4 hours da day/
	
B.	Humidity:	10% to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum housing; polycarbonate sunshield, coated 
                                             glass lens cover
B.	Dimensions:	Height: 14.2 in. (361.9 mm), 
Diameter: 7.5 in. (190 mm)
C.	Weight: 	11 lb (5 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	1.5” NPT pipe interface. Mounting accessories available 
B.	Adjustments:	Pan 360° continuous; tilt: -20° - 90° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10/100/1000 Base-T, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	3840x2160, 2560x1440, 1920x1080, 1280x960/720, 720x408, 640x360
Max 30/25 fps @ 4K max resolution
F.	Web Browser:	Safari, Firefox, Google Chrome, Microsoft Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             3 DNR; motion detection (5 zones); day/night mode; 
                                             white balance, AGC; Electronic Shutter, automatic or 
                                             manual; digital zoom; privacy masks (32);OIS; 
                                             motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:	Tampering, Motion, Intrusion, Line Cross, Tailgating, 
                                             Loitering and Crowd Detection, Auto-Tracking (people); 
                                             Museum Search in Valerus VMS.
J.	Supported Protocols:	IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, FTP, ICMP, LDAP,
                                             NTP, DHCP, DNS, DDNS, UDP, QoS, SSL 1.1.G, 
                                            TLS 1.2, Zeroconfig, Bonjour, Firewall, 802.1x, 
                                            ONVIFS/G/T/M

2.09	CERTIFICATIONS

A.	CE
B.	UL (pending)
C.	FCC, Class A
D.	IP66
E.	IK10
F.	ONVIF S/T/G/M
G.	RoHS
H.	NDAA/GSA/TAA compliant

2.10	WARRANTY

A.	5 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP PTZ dome camera shall be Vicon Industries V2008PTZ-IR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.