Vicon® Industries Inc		VALERUS VICONNET GATEWAY		
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE
PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components, regularly manufactured, 
regularly utilized in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24-hour 
immediate technical assistance for either the dealer/installer at no charge.

D.	All systems and components shall be provided with an explicit manufacturer warranty.

2.02	DIGITAL VIDEO SOLUTION FOR LEGACY AND CURRENT VMS – GENERAL 

A.	The Gateway Software shall be a solution that shall meet the requirements of business and government surveillance applications to preserve use of their legacy VMS. 

B.	The Gateway shall be a separate module designed to allow bridging the existing ViconNet system to a Valerus VMS.

C.	The Gateway shall be a separate installation that shall be available for the Valerus VMS at a minimum of version 18. The existing ViconNet VMS shall be at a minimum of 5.6d.

D.	The Gateway shall require a license per each Gateway PC.

E.	The software shall run on a COTS PCs with a minimum of Intel Core i7 processor, 16 GB of RAM. The software shall run on the Microsoft® Windows® 10 64-bit. The Gateway shall also be available pre-installed on manufacturer certified hardware.

F.	In Valerus systems where a dedicated Application Server is used, the Gateway can run on that 
	computer and support up to 75 ViconNet video channels. For ViconNet systems with more than 
	75 video channels, a dedicated Gateway PC shall be required to run the Gateway. The Gateway 
	computer must run on a 1 Gbps network.

2.03	GATEWAY CAPABILITIES

A.	The Gateway shall connect to a ViconNet system and shall bridge a camera group that is set up in the ViconNet Nucleus.

B.	Video and audio shall be pulled from the ViconNet VMS and sent to the Valerus clients transparently. The channels shall be handled by the Gateway and stream through it. On Valerus, the video and audio channels shall appear as any other resource; they shall be able to be used exactly as if they are an IP camera connected directly to Valerus.

C.	Functionality supported through the Gateway shall include:

1.	 Live video/audio viewing that shall be able to be used in tours and views
2.	Playback of video/audio recorded on the ViconNet devices
3.	Control of PTZ cameras on the ViconNet devices.
4.	Dewarp supported 360° cameras on the ViocnNet system.
5.	Thumbnail and Museum Search of video recorded on the ViconNet devices.
6.	Export through the Valerus interface.
7.	Each Gateway shall be able to support up to 500 ViconNet video channels; using multiple Gateways shall be supported.

D.	All recordings and recording settings shall still be on ViconNet. Events shall only trigger on ViconNet. 

2.04	ELECTRICAL SPECIFICATIONS

A.		Input Voltage:	105-240 ±10% VAC, 50/60 Hz.	
B.		Current:	0.66 A @ 115VAC; 0.33 A @ 240 VAC.	
C.		Power Consumption:  	
76 W	
D.		CPU	Intel® Core™ i7. 	
E.		RAM Memory	16 GB minimum.	
F.		Heat Output:  	266 btu/hour. 	
G.		Operating System:	Microsoft Windows 10 LTSB.	
H.		LAN Interface:	100/1000 Base T Ethernet interface on main board.	
I.		Front Panel
Controls/Indicators:	
Power, network activity LEDs, USBs.	
J.		Certifications:	FCC Class A.	

2.05	MECHANICAL SPECIFICATIONS

A.		Application:	Indoor.	
B.		Mounting:	Desktop or rack unit mounted in a standard EIA compliant rack, 19 in. (483 mm) wide opening. Rack height is 1.75 in. (44 mm) or 1 RU.	
C.		Dimensions-Rack:  	Width (W): 19.0 in. (483 mm).
Depth (D): 16 in. (406mm).
Height (H): 1.75 in. (44.45 mm), 1 RU.	
D.		Dimensions-Desktop	Desktop: Width (W): 3.75 in. (95.25 mm).
        Depth (D): 10.5 in. (266.7 mm).
        Height (H): 9.5 in. (241.3 mm).	
E.		Weight-Rack:	18.2 lb. (8.3 kg) approximately.	
F.		Weight- Desktop:	8.1 lb. (3.7 kg) approximately.	
G.		Construction:	Steel and plastic.	
H.		Color:	Black.	

2.06	ENVIRONMENTAL SPECIFICATIONS

A.	Operating 
Temperature Range:	
32 to 104ºF (0 to 40ºC).	
B.	Operating 
Humidity Range:	
0 to 95%, non-condensing.	

2.07	WARRANTY
A.	3 years, parts and labor.

2.08	APPROVED MANUFACTURERS

A.	The Gateway Solution shall be Vicon’s Valerus-ViconNet Gateway. The Gateway Server preloaded with Gateway and required ViconNet software shall be models VLR-VN-GW (desk-top) and VLR-VN-GW-RK (rack-mount). The license for Gateway shall be model VLR-VN-GW-LIC and the upgrade license for existing Valerus systems shall be VLR-VN-GW-LIC-ADD.

END OF SECTION

Vicon and its logo are registered trademarks of Vicon Industries Inc in the United States and other countries. 
Valerus and its logo are trademarks of Vicon Industries Inc.
Microsoft and Microsoft Windows are registered trademarks of Microsoft Corporation in the United States and other countries.
Intel and Core are registered trademarks of Intel Corporation in the United States and other countries.