Vicon® Industries Inc		VALERUS VIDEO MANAGEMENT SOFTWARE		
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE
PART  2  	PRODUCTS
2.1	GENERAL
A.	All equipment and materials used shall be standard components, regularly manufactured, 
regularly utilized in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll free 24-hour 
immediate technical assistance for either the dealer/installer at no charge.
D.	All systems and components shall be provided with an explicit manufacturer warranty.
E.	All Cameras, NVRs, DVRs, and Workstations shall be available to be shipped pre-configured and programmed to the systems requirements by the manufacturer.
2.2	VIDEO MANAGEMENT SYSTEM
A.	Basis of Design:  Valerus Video Management System as manufactured by Vicon Industries.
1.	Digital Video Recording Management and Network Software – General:
a.	Video Management Software (VMS):  Browser-based application meeting requirements of business and government surveillance applications.
1)	Web client with single point of management for entire system.
2)	Configuration Sections of Application:  Add, configure and operate recording servers, application servers, web servers, as well as IP cameras and encoders (edge devices).
3)	Operation and Maintenance Application:  Complete and comprehensive for video surveillance system.
4)	Full live digital video and audio surveillance over a standard 1 Gbps network.
b.	The VMS shall support recording, playback and archiving of video in standard industry compression formats, including H.265, H.264 and M-JPEG.
c.	True Open Standards (ONVIF) as Basis:  Thin client architecture. Centrally licensed. COTS compatible software or available preloaded on a manufacturer certified application/web server or recording server (NVR).
1)	A Desktop Client solution shall be available for those users who prefer not to work in a browser environment.
d.	Two License Tiers:  Associated with number of edge devices and a specific feature set. Licensing shall be based on a per edge device basis.
e.	COTS PCs with a minimum of Intel Core 7700 i7 processor, 16 GB of RAM and 5 GB of disk space for installation and a minimum of 75 GB of disk space for a recording device.
1)	Operating System:  Microsoft Windows 10 64-bit, 
2)	Operating System:  Microsoft Windows 2016, 2019 and 2022 64-bit Server.
3)	The Client (web) supports Windows 7 Operating systems.
f.	Software Features:  Easy to Use Tabs:  Access configuration screen and dashboard monitoring systems health. Monitoring Screen:  Video display area with available resources list. Multiple Display Views:  Configurable with variety layouts. Multiple Monitors:  Supported.
g.	Live Video:  Stream through Recording Server (NVR) with auto fail over to cameras. PTZ available from live video. Presets and tours are configurable. Digital zoom provided on video displays. 
h.	Web Based Interface:  
1)	Access the VMS from any standard web browser enabled device.
2)	Browser compatibility:  Microsoft Edge. Chrome shall be able to be used with the Valerus Chrome extension from the Chrome store.
3)	Provide live viewing, playback and PTZ controls. 
4)	Mobile App:  Apple and Android smart phones and tablets. View live or recorded video. View concurrent multiple video streams; 4 on phones, 9 on tablets. Full control of PTZ, including presets. Quick and simple playback. Pinch to zoom on live and recorded video.
i.	Export Icon:  Easy access on display to save a video clip. Archived in MP4 format and authenticated in the player per the ONVF spec. 
j.	Playback:  Supported from main screen without leaving live video viewing area. Clicking Playback from time icon will allow selecting the playback to start from a specific date and time using standard calendar tools.
k.	Software Delivery:  Provided on manufacturer’s website.
l.	Events:  Setup in configuration area. Pre-Event Recording:  Supported and with event notification.
m.	Access Control System Support:  Accessed using a simple tab click. Interface opens in popup window that can be used in conjunction with the VMS. 
n.	Enhanced Edge-based Analytics:  Show bounding boxes around detected objects in live and playback video.
o.	Authorization roles shall be configurable; these roles shall then be listed in the Resources list on the monitoring display screen. This Resources list can be viewed in a hierarchy view with these groups or as a flat list.
p.	Video Masking:  Available centrally through the VMS. Allow users with the correct authority to unmask video as needed using icon on the display screen. Unmask feature available on live and playback video.
q.	Quick Configuration Wizard:  Streamlined process for typical and basic system setup with minimal input required.
r.	Search Functions:  Six search functions available including museum search (supports AI classification for those cameras with that functionality), thumbnail search, events framework search, event/alarm search, audit log and Analytics Search. Additionally, the player shall support colored bounding boxes with for the AI analytics, person (green box), vehicle (cyan/blue box) and animal (yellow box).
s.	Capability for 360 degree lens dewarp available for use with cameras with fisheye lenses.
t.	Integration with Active Directory (AD):  Allow user management via the AD.
u.	Override mode:  Allows operating in case AD communication is lost.
v.	Import user list: A user list can be prepared in advance in standard Excel sheet saved in .csv format and imported into Valerus VMS.
w.	Auto Archive:  Archiving can be set up to occur on a schedule, for either all data or only events-based recording, to local or network/cloud storage.
x.	Multi-language Support:  All text in the user interface translated to selected language.
y.	Backup and Restore for system settings shall be available. Backup can be to a network drive or cloud storage.
z.	Keypads and PLC controls supported. Numeric IDs for devices configurable for use with controls. These devices shall be able to control remote monitors.
aa.	Central Software Upgrade Interface:  Provides the ability to upgrade the entire system by pushing the upgrade from the Application Server to all devices on the system.
bb.	System supports IPv4/IPv6 and HTTPS. There shall be HTTPS support for External Events.
cc.	A Gateway module shall be available to bridge migration from a legacy ViconNet Video Management System to this VMS and use the old system resources.
dd.	The system shall have built in Log Collection from all system PCs, making it easier to troubleshoot problems. An advanced tool shall be provided.
ee.	The system shall accept external text strings from third party systems.
ff.	Alarm notification shall be both visual and audible. The display of the alarm tab view can be auto-dismissed after a set time and return to the previous view; the alarm tab view can still be accessed as needed. Live view from up to four cameras shall be able to display in the alarm tab. Multiple alarms (external events only) shall be able to be imported in a single action using an Excel sheet template. A Test Email button shall be provided within the interface.
gg.	A Report button shall generate an Excel or HTML report of the devices sorted by their hosting NVRs or a flat list.
hh.	Devices shall be able to be replaced or moved, for load balancing purposes.
ii.	Storage of video and exports can be mapped to another server, a NAS on the network or to the cloud (AWS/Wasabi).
jj.	An NVR Failover unit shall be able to be configured to take over in the event of an NVR failure.
kk.	A Mapping function shall be provided that allows the placement of resource devices on any imported map. The map shall be either a static or live map. The device icons on the map shall be adjustable in size.
ll.	An Events Database shall exist to store any event that occurs in the system. From the Event Search screen, a query shall be able to be created to search for any event that occurs on the system from any resource in the system.
mm.	A video clip, either in live or playback, shall be able to be bookmarked for easy referral.
nn.	The ability to use mobile devices as mobile cameras shall be available. The mobile device shall be able to receive event alerts.
oo.	The VMS shall be able to accept partner systems through an integration framework. These partner resources will show on the Resources list and can display in a tile.
pp.	A Snapshot function shall be provided to capture video from live or playback; this snapshot shall be able to be saved. It shall be possible to capture snapshots from all resources and update them all at the same time.
qq.	An Audit Log shall be available to track every user’s actions.
rr.	Keypads/PLC shall have the ability to call up other remote monitors. 
ss.	A thick-client solution shall be available for users who don’t want to use a browser.
tt.	Shall be operational in a virtual environment.
uu.	An integration framework shall be provided to allow partnerships with third party systems such as LPR and Access Control.
vv.	An Alarms Management module shall be provided that shall allow events to be defined as alarms and provide tools to review open alarms and close them. Alarms shall have a defined life cycle and procedures shall be able to be created to handle these alarms, if needed.
ww.	A Client Performance Indicator shall be provided to indicate system performance as more cameras are added and displayed.
xx.	Monitors can be managed from the Application Server in a central way and a monitor can be defined as an alarm monitor for use by the alarms/rules in the system. Monitor IDs can be synced.
yy.	Virtual Matrix Display Controller (VMDC) feature shall be available for user to take control of any client workstation on the same network. User shall be able to view and display video on those remote monitors.
zz.	The system shall have an enhanced dashboard that shall present the system’s health status and provide health monitoring information and statistics on all connected devices, including Application Server, NVRs and cameras. It shall provide notifications that notifications that provide cyber security and an easy-to-use activity mapping chart.
2.	Setup, Configuration and Security of VMS:
a.	Multi-User Authorization Login Application. 
1)	Offer levels of authorization based on functions. 
b.	Setup Utility:  Allows Administrator to configure additional users as well as user groups. 
1)	User authorization:  Configurable for specific system operations. Authorization Permission Setup:  Performed using the User screen. 
2)	Authorization Roles:  Available to configure from the Authorization Roles screen. Permissions:  Provide authority to perform all system functions. 
3)	Users and groups on AD servers may be imported and become a group in the VMS.
4)	The software shall offer a full multi-user authorization process as follows:  Authorization Roles:  Created once globally. Authorized and given specific permissions. Users:  Created once globally and may be given rights to groups. No virtual limit on number of groups and users authorized in the software. Authorization Roles to be authorized or denied access to:  Monitoring screen for video display. Configuration. Dashboard. Video and audio (media) export. Override masking. Override View.
c.	A user, given appropriate access, may remotely configure components connected to the network. An access list shall be able to be created to add those PCs that are allowed to connect to Valerus, adding another layer of security.
d.	Software permits viewing of live video from any edge device connected to any recording server on the network.
e.	Export Icon:  Simplifies process of exporting video and creating archives and saving video to media, such as:  USBs, CD, DVDs or solid-state drives. An embedded player shall be optional with each exported/archived video clip for playback on any machine if configured to do so.
f.	Event Rules:  Create rules triggered by an event occurrence. Define actions executed for a given event. Events are selectable. Rules are configurable after an event is selected.
g.	Event Association:  Multiple devices may be associated with an event. Actions Triggered by Event:  Configurable as On and Off. Display live video. Display a view. Go to a preset. Operate a relay. Run a PTZ tour. Run a view tour. Start a URL. Delay function.
h.	Scheduled Recordings:  Applies to cameras, encoders and microphones. Scheduling is based on rules configurable for actions the system takes upon an event. Schedules accessible on recording tab in device configuration. Create and Schedule Recordings:  By authorized users. How often schedules repeat; weekly, monthly, yearly or never. Determines how the systems prioritizes schedules if schedule times overlap. Schedules available when configuring recording and rules, saving the need to create multiple and duplicate schedules. Sequencing cameras, including multi-screen displays. Record cameras at different qualities and frame rates from any recorder on the network. Schedule shall allow running preconfigured combinations of camera, sensor and PTZ programmed routines.
i.	System Components:  Application/Web Server:  Act as main system server; Windows based. Global configuration of the system is stored on this server. Recording Servers (NVRs):  Windows based providing communication, live streaming, recording, video playback and audio from cameras and encoders.
j.	Device Configuration:  Valid devices to be configurable for system recognition and operation. Cameras, fixed or with integrated PTZ. Microphones. Encoders. Sensors. Relays.
k.	Authentication:  Video from cameras is enabled to verify the authentication of the video and present an authentication symbol on the displayed video for recorded playback through the player when enabled only on export.
3.	User Interface for VMS:
a.	User Friendly Tabs:  Allow monitoring of live and playback video, and configuration of the system.
b.	Login Window:  Consists of User Name and Password fields. Default User Name and Password:  Available for initial login. Configurable for increased security; there shall be an option to enforce a complex password.
c.	Serve operators, supervisors and system administrators. 
d.	Monitoring Display Screen:  
1)	Selection of number of tiles to display. 
2)	Resource list of devices in system. Viewable as flat list or hierarchical list based on user configured groups. Resources include names of devices and icons depicting devices. Video Channels (cameras) connected, differentiating between PTZ and fixed cameras. Audio Channels (microphones). Views. Tours. Web Pages. Relay Outputs.
3)	Display Area:  Offers display configurations up to 36 tiles. Full screen View:  Available. More views added by clicking the plus sign to create new view tabs while not losing the default view. Controls:  Change the layout. Stop all displays. Export. Synchronize playback. Control current selected tab.
4)	Camera Controls:  Display at top of a tile when mouse hovers and may be locked in place. Playback. PTZ control. Digital zoom. Unmask. Export. Configuration settings
5)	Playback controls:  Visible when cameras go to playback. Looping a video section. Slow mode. Play from time. Rewind, fast rewind, pause, forward, and fast forward. Back to live video and current time.
6)	Access to all available programming menus.
7)	Viewing live devices is performed by dragging a device to any tile. Audio devices display in a smaller area below the video tiles.
e.	Dashboard, Search, Alarms and Configuration Menu Access:  Clicking a tab at the top of the screen.
4.	Video Quality for VMS:  Support any resolution video, jpeg and H.264 compression.
5.	Add-Ins for VMS
a.	Access Control Systems:  Available for integration.
1)	Meet requirements of business and government access control systems.
2)	Monitor and control facility access as well as video detection, temperature and communications loss monitoring.
3)	Provide control and access to users on Local Area Networks (LAN), Wide Area Networks (WAN), wireless networks and the Internet.
4)	Video viewing playback and PTZ control from the VMS.
b.	A method to add partner systems shall be provided through an integration framework. It shall support VAX Access Control, Vicon LPR, Neural Lab LPR and Thermal Radar sensor.
1)	When integrating with the VAX Access Control System, digital inputs, relay outputs and action plans created in VAX shall be automatically added in Valerus to be configured as any other Resource. Doors shall be able to be edited and user information on the cardholder picture shall be updated once updated in VAX.
2)	Rules can be configured based on these partner resources and then alarm events shall be able to be created and then searched for.
3)	The partner icons can also be added to maps.
B.	Basis of Design:  Valerus Shadow Elite Server System as manufactured by Vicon Industries.
1.	Digital Servers:  Preloaded with Valerus VMS. 
a.	Application Servers:  VEAA-1U00N0-00 (1U rack-mount)
b.	Recording Servers:  VERA-SFXXN0-00 (preloaded small desk-top, i5 processor)
c.	Recording Servers:  VERA-1UXXN0-XX (preloaded 1U rack-mount, Xeon processor).
d.	Recording Servers with RAID5: VERA-1UXXR5-XX (preloaded 1U rack-mount, Xeon processor).
e.	Recording Servers with RAID5:  VERA-2UXXR5-XX (preloaded 2U rack-mount, Xeon processor).
f.	Recording Servers with RAID6:  VERA-2UXXR6-XX (preloaded 2U rack-mount, Xeon processor).
g.	Client Workstations:  VECA-MC00N0-00 (micro desk-top, i7 processor).
h.	Client Workstations:  VECA-SF00N0-00 (small form factor desk-top, i5 processor).
i.	Client Workstations:  VECA-1U00N0-00 (1U rack-mount, Xeon processor)
j.	Certifications:  UL, CE, FCC Class A. Servers shall be powered by Dell and Intel technology and backed Dell NBD onsite support, 24/7 customer service and 5 year warranty 
k.	Application, Client Workstations and Recording (NVR) Servers. 
1)	Operating System:  Microsoft Windows 10 Enterprise IoT. 
2)	Processor shall be model dependent. Intel Core i7 processor, Xeon processors shall be available. Memory: 16 GB RAM (Core i7/Xeon models). USB ports. Monitor outputs.
l.	Server Housing:  Desktop (micro/small form factor) or rack-mount case (1U or 2U) with all suitable connectors available on the back panel. 
m.	Number of cameras supported, storage capacity and max data rate shall depend on model selected; models shall be available that support up to 250 cameras, 800 Mbps data rate and 520 TB storage.
n.	Server Capacities:
1)	Elite Recording Server Storage Capacity:  internal 8 TB hard-drive.
2)	Elite Recording Server Storage Capacity:  internal 16 TB hard-drive.
3)	Elite Recording Server Storage Capacity:  internal 20 TB hard-drive
4)	Elite Recording Server Storage Capacity:  internal 24 TB hard-drive
5)	Elite Recording Server Storage Capacity:  internal 32 TB hard-drive.
6)	Application Server:  Standalone unit with no storage capability.
7)	Application Server:  All-in-one unit included in the recording server.
8)	Elite Internal Raid5 Storage Device:  48 TB storage capacity.
9)	Elite Internal Raid5 Storage Device:  64 TB storage capacity.
10)	Elite Internal Raid5 Storage Device:  80 TB storage capacity.
11)	Elite Internal Raid5 Storage Device:  84 TB storage capacity.
12)	Elite Internal Raid5 Storage Device:  96 TB storage capacity.
13)	Elite Internal Raid5 Storage Device:  120 TB storage capacity.
14)	Elite Internal Raid5 Storage Device:  140 TB storage capacity.
15)	Elite Internal Raid5 Storage Device:  160 TB storage capacity.
16)	Elite Internal Raid5 Storage Device:  180 TB storage capacity
17)	Elite Internal Raid5 Storage Device:  200 TB storage capacity.
18)	Elite Internal Raid5 Storage Device:  220 TB storage capacity
19)	Elite Internal Raid5 Storage Device:  240 TB storage capacity.
20)	Elite Internal Raid6 Storage Device:  280 TB storage capacity.
21)	Elite Internal Raid6 Storage Device:  300 TB storage capacity.
22)	Elite Internal Raid6 Storage Device:  320 TB storage capacity.
23)	Elite Internal Raid6 Storage Device:  340 TB storage capacity.
24)	Elite Internal Raid6 Storage Device:  360 TB storage capacity.
25)	Elite Internal Raid6 Storage Device:  380 TB storage capacity.
26)	Elite Internal Raid6 Storage Device:  400 TB storage capacity.
27)	Elite Internal Raid6 Storage Device:  420 TB storage capacity.
28)	Elite Internal Raid6 Storage Device:  440 TB storage capacity.
29)	Elite Internal Raid6 Storage Device:  460 TB storage capacity.
30)	Elite Internal Raid6 Storage Device:  480 TB storage capacity.
31)	Elite Internal Raid6 Storage Device:  500 TB storage capacity.
32)	Elite Internal Raid6 Storage Device:  520 TB storage capacity.
o.	Application Servers.
p.	Specifications for Elite Digital Application Servers:
1)	Application Servers
a)	Model:  VEAA-1U00N0-00. 1U rack.
b)	Certifications:  FCC Class A.
c)	Power Supply:  
1)	1U Rack:  550 W, dual redundant.
d)	Typical Power Consumption:  100 W (350 BTU).
e)	Max Power Consumption:  
1)	1U Rack:  220 W (750 BTU) max.
f)	CPU:  
1)	1U Rack:  Xeon E-22XX 16 GB DDR4.
g)	OS Drive:  256 GB M.2 NVMe SSD.
h)	Display:  
1)	USB-C.
i)	Operating System:  Microsoft Windows 10 Iot Enterprise.
j)	Networking:  
1)	1U Rack:  1x 1GbE RJ-45, Intel i219 or 1x 10GbE RJ-45, Aquantia.
k)	Front Panel Controls/Indicators:  
1)	USBs (1x USB 3.1 C/2x USB 3.1), Headphone; 1x SD card reader.
l)	Rear Panel I/O and Controls:  
1)	AC power socket; 2x USB-C; 1x serial; 2x RJ-45.
m)	Mechanical Specifications:
1)	Application:  Indoor. Construction:  Steel and plastic.
2)	Mounting:  
a)	Rack Mount:  1U rack.
3)	1U Rack (HxWxD):  1.7 x 19 x 23.19 inches (43 x 483 x 589 mm) (with bezel).
a)	Weight:  19.27 lbs (8.74 kg).
n)	Environmental Specifications:
1)	Operating Temperature Range:  50 to 95 degrees F (10 to 35 degrees C).
2)	Operating Humidity Range:  10 to 85 percent, non-condensing.
3)	Warranty:  5 years, Parts, and labor.
2)	Client Workstations: Available with 2 or 4 or monitor outputs:
a)	Model:  VECA-MC00N0-00. Micro form factor. 
b)	Model:  VECA-SF00N0-00. Small form factor. 
c)	Model:  VECA-1U00N0-00. 1U rack.
d)	Electrical Specifications:
1)	Certifications:  FCC, Class A.
2)	Power Supply:
a)	Micro:  65 W external PSU. 
b)	Small Form Factor:  200 W. 
c)	1U Rack:  550 W (dual redundant).
3)	Typical Power Consumption:  
a)	Micro:  60 W (200 BTU).
b)	Small Form Factor: 200 W (650 BTU).
c)	1U Rack:  100 W (350 BTU).
4)	Max Power Consumption:  
a)	Micro:  120 W (400 BTU).
b)	Small Form Factor:  300 W (1000 BTU).
c)	1U Rack:  220 W (750 BTU).
5)	CPU:  
a)	Micro:  Intel Core i7 10th Gen 16 GB DDR4.
b)	Small Form Factor: Intel Core i5 12th Gen 16 GB DDR4.
c)	1U Rack:  Intel Core Xeon E-22XXG, 16 GB DDR4.
6)	OS Drive:  256 GB SSD.
7)	Display:  
a)	Micro:  Intel HD (HDMI + DP); supports dual 4K monitor.
b)	Small Form Factor:  Intel HD (3x DP; 1x HDMI); supports quad 4K monitor.
c)	1U Rack:  Nvidia Quadro (4x mini-DP); supports quad 4K monitors.
8)	Operating System:  Microsoft Windows 10 Iot Enterprise.
9)	Networking:  
a)	Micro/Small Form Factor:  1x 1GbE RJ-45.
b)	1U Rack:  1x 1GbE RJ-45, Intel i219 or 1x 10GbE RJ-45, Aquantia.
10)	Front Panel Controls and Indicators:  
a)	Micro:  USBs (1x USB 3.2, 1x USB3.2-C); 1x Line out; Headphone.
b)	Small Form Factor:  USBs (1x USB C/1x USB 3/1x USB 2.0); 1x Audio Port; 1X Kensington lock.
c)	1U Rack:  USBs (1x USB 3.1-C/2x USB 3.1); 1x Headphone; 1x SD card reader.
11)	Rear Panel I/O and Controls:  
a)	Micro:  1x RJ-45; display ports (HDMI + DP); USBs (4x USB 3.2); Kensington lock.
b)	Small Form Factor:  AC power socket; USBs (4x USB 3.2, 2x USB 2.0); 1x RJ-45, line out; 3x DP/1x HDMI display ports; Kensington lock.
c)	1U Rack:  AC power socket; 2x USB Type-C, 1x serial; USB-C display port.
e)	Mechanical Specifications
1)	Micro Desktop: (HxWxD):  7.17 x 1.42 x 7.02 inches (182 x 36 x 178.6 mm). Weight:  2.56 lb. (1.16 kg).
2)	Small Form Factor Desktop: (HxWxD):  11.42 x 3.65 x 11.53 inches (290 x 93 x 293 mm). Weight:  8.44 lb. (3.83 kg). 
3)	1U Rack (HxWxD): 1.7 x 19 x 23.19 inches (43 x 483 x 589 mm) (with bezel). Weight:  19.3 lb. (8.73 kg).
f)	Environmental Specifications:
1)	Operating Temperature Range:  
a)	Micro/1U: 50 to 95 degrees F (10 to 35 degrees C).
b)	Small Form Factor: 50 to 113 degrees F (10 to 45 degrees C).
2)	Operating Humidity Range:
a)	Micro/ Small Form Factor:  20 to 80 percent, non-condensing.
b)	1U Rack:  10 to 85 percent, non-condensing.
g)	Warranty:  5 years, parts, and labor.
3)	Recording Servers:
a)	NON-RAID Recording Servers
1)	Model VERA-SFXXN0-XX, Small Form Factor.
2)	Model VERA-1UXXN0-XX, 1U Rack. 
3)	Electrical Specifications:
4)	Certifications:  FCC, Class A.
5)	Power Supply:
a)	Small Form Factor: 200 W.
b)	1U Rack:  Xeon: 550 W, dual redundant.
6)	Typical Power Consumption:
a)	Small Form Factor: 200 W (650 BTU).
b)	1U Rack: 100 W (350 BTU).
7)	Maximum Power Consumption:
a)	Small Form Factor: 300 W (1000 BTU).
b)	1U Rack:  220 W (750 BTU).
8)	CPU:
a)	Small Form Factor: Intel Core i5 12th Gen 16 GB DDR4.
b)	1U Rack:  Xeon E-22XX 16 GB DDR4.
9)	OS Drive:  256 GB M.2 NVMe SSD.
10)	Data Drive Configuration:  SATA. 
11)	Display:	  
a)	Small Form Factor: Intel HD. 3x DP/1x HDMI; supports quad 4K monitor. 
b)	1U Rack:  Nvidia Quadro, 4x mini-DP; supports quad 4K monitors.
12)	Operating System:  Microsoft Windows 10 Iot Enterprise.
13)	Networking:
a)	Small Form Factor: 1x 1GbE RJ-45, Intel 82574. 
b)	1U Rack:  1x 1GbE RJ-45, Intel i219 
c)	1U Rack:  1x 10GbE RJ-45, Aquantia. 
14)	Front Panel Controls and Indicators:  
a)	Small Form Factor:  1x USB 3.2 C/1x USB 3.2/2x USB 2.0; Headphone. 
b)	1U Rack: 1x USB 3.1 C/2x USB 3.1; Headphone; 1x SD card reader.
15)	Rear Panel I/O and Controls:
a)	Small Form Factor:  AC power socket; USBs:  4x USB 3.2, 2x USB 2.0); 1x RJ-45, line in and line out; Display ports:  3x DP/1x HDMI; Kensington lock.
b)	1U Rack:  AC power socket; 2x USB:  Type-C, 1x serial:  1x RJ-45; 4x Mini-DP display ports.
16)	Mechanical Specifications:
a)	Application:  Indoor.
b)	Mounting:  
1.	Desktop:  Small Form Factor (HxWxD): 11.42 x 3.65 x 11.53 inches (290 x 93 x 293 mm). Weight:  8.44 lb. (3.83 kg). 
2.	Rack Mount:  1U Rack (HxWxD): 1.75 x19 x 23.19 inches (44.5 x 483 x 589 mm). 
Weight:  42.6 lbs (19.3 kg).
c)	Construction:  Steel and plastic.
17)	Environmental Specifications:
a)	Operating Temperature Range:
1)	Small Form Factor:  50 to 113 degrees F (10 to 45 degrees C).
2)	1U Rack: 50 to 95 degrees F (10 to 35 degrees C).
b)	Operating Humidity Range:
1.	Small Form Factor:  20 to 80 percent, non-condensing.
2.	1U Rack: 10 to 85 percent, non-condensing.
18)	Warranty:  5 years parts and labor.
4)	RAID Recording Servers (NVRS):  
a)	Model VERA-1UXXXR5-XX:  1U rack, RAID 5. 
b)	Model VERA-2UXXXR5-XX:  2U rack, RAID 5.
c)	Model VERA-2UXXXR6-XX:  2U rack, RAID 6.
d)	Electrical Specifications:
1)	Certifications:  FCC Class A.
2)	Power Supply:  
a)	1U RAID5 Rack:  600 W, dual redundant.
b)	2U RAID5 Rack:  800 W dual redundant.
c)	2U RAID6 Rack:  1100 W dual redundant.
3)	Typical Power Consumption:
a)	1U RAID5 Rack:  250 W (850 BTU).
b)	2U RAID5 Rack:  400 W (1365 BTU).
c)	2U RAID6 Rack:  370 W (1300 BTU).
4)	Max Power Consumption:
a)	1U RAID5 Rack:  300 W (1000 BTU).
b)	2U RAID5 Rack:  550 W (1800 BTU).
c)	2U RAID6 Rack:  420 W (1500 BTU).
5)	CPU:
a)	1U RAID5 Rack:  Xeon, 16 GB ECC DDR4.
b)	2U RAID5 Rack:  Xeon, 16 GB ECC DDR4.
c)	2U RAID6 Rack: Xeon, 32 GB ECC DDR4
6)	OS Drive:
a)	1U RAID5/2U RAID5 Rack:  2x 240 GB M.2 SSD (RAID-1).
b)	2U RAID6 Rack 480 GB M.2 SSD (RAID-1).
7)	Data Drive Configuration:  
a)	1U Rack:  RAID5.
b)	2U Rack:  RAID5.
c)	2U Rack:  RAID6.
8)	Display:  
a)	1U RAID5/2U RAID5/2U RAID6 Rack:  Single VGA, 1920x1200 (WUXGA) max.
9)	Operating System:  Microsoft Windows 10 Iot Enterprise.
10)	Networking:  
a)	1U/2U RAID5 Rack:  2x 1GbE; 1x RJ-45 iDRAC.
b)	2U RAID6 Rack:  4x 1GbE Broadcom NetExtreme 5720; 2x 10GbE BaseT; 1x RJ-45 iDRAC.
11)	Front Panel Controls/Indicators:
a)	1U RAID5:  1x USB 2.0; 1x micro USB for iDRAC.
b)	2U RAID5:  1x USB 2.0; 1x micro USB for iDRAC; 1x VGA.
c)	2U RAID6:  1x USB 2.0; 1x micro USB for iDRAC with LED; system health/system ID LEDs.
12)	Rear Panel I/O and Controls:
a)	1U RAID5 Rack:  AC power socket; 2x USB 3.0, 1x serial; 1x VGA, 1x RJ-45 iDRAC, 2x RJ-45.
b)	2U RAID5 Rack:  AC power socket; 1x USB 2.0, 1x USB 3.0, 1x VGA, 1x RJ-45 iDRAC, 2x RJ-45.
c)	2U RAID6 Rack:  AC power socket; 1x USB 2.0, 1x VGA; 1x RJ-45 iDRAC; 4x RJ-45; 2x 10 GbE BaseT.
e)	Mechanical Specifications:
1)	Application:  Indoor.
2)	Mounting:  Rack mount (1U RAID5/2U RAID5/2U RAID6).
3)	Dimensions (HxWxD):
a)	1U RAID5 Rack:  1.7 x 19 x 23.58 inches (43 x 483 x 598.9 mm) (with bezel).
b)	2U RAID5 Rack:  3.5 x 19 x 28.4 inches (89 x 483 x 721.6 mm) (with bezel).
c)	2U RAID6 Rack:  3.4 x 19 x 34.4 inches (86.8 x 483 x 872.7mm).
4)	Weight:
a)	1U RAID5 Rack:  29.98 lbs (13.6 kg).
b)	2U RAID5 Rack:  65.4 lbs (29.7 kg).
c)	2U Rack RAID6:  102.1 lbs (46.3 kg).
5)	Construction:  Steel and plastic.
f)	Environmental Specifications:
1)	Operating Temperature Range:  
a)	1U RAID5 Rack:  50 to 95 degrees F (10 to 35 degrees C).
b)	2U RAID5 Rack: 73 to 95 degrees F (23 to 35 degrees C).
c)	2U RAID6 Rack:  41 to 104 degrees F (5 to 40 degrees C). 
2)	Operating Humidity Range:  
a)	1U RAID5 Rack:  5 to 95 percent, non-condensing.
b)	2U RAID5/2U RAID6 Rack:  5 to 85 percent, non-condensing.
g)	Warranty:  5 years, parts, and labor.

2.3	CAMERAS FOR VIDEO MANAGEMENT SYSTEMS
A.	General:
1.	All equipment and materials used shall be standard components, regularly manufactured, regularly utilized in the manufacturer’s system.
2.	All systems and components shall have been thoroughly tested and proven in actual use.
3.	All systems and components shall be provided with the availability of a toll free 24-hour immediate technical assistance for the dealer/installer at no charge.
B.	LPR Cameras
1.	Basis of Design: V2008B-W310-LPR, V2008B-W818-LPR bullet cameras and V2008-W0950-LPR box camera kit License Plate Recognition IP Network Camera as manufactured and supplied by Vicon Industries.
a.	Certifications:  CE, FCC Class A, ONVIF S/T/G/Q, RoHS, NDAA/GSA/TSA compliant. Bullet camera model shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance, including front glass. The box camera kit shall be IP68 rated and IK10 rated for impact resistance.
b.	General Features
1)	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
2)	Systems and Components:  Tested and proven in actual use.
3)	Technical Support: Toll free 24-hour technical support phone number
from the manufacturer. No charge service for dealers and installers.
4)	Provided with an explicit 5-year manufacturer warranty.
5)	The LPR software shall allow capture, storing and searching on an unlimited number of license plates and allow examination of details such as vehicle color, make and model. Customized lists of license plates shall be able to be created to generate an alert; lists shall be able to be synchronized from one camera to other cameras on the system. On-screen alarm handling procedures shall provide step-by-step instructions for addressing alarms. License plates from over 70 countries shall be supported. The ability to search by plate shall be available. Having the LPR analytic on the edge shall allow for a standalone LPR solution for users who do not want to integrate with a compatible VMS; it shall be able to integrate with the manufacturer’s video management system to monitor events through its Alarms Management suite. When the LPR camera is used with Valerus, the powerful alarm handling procedures shall give you step-by-step instructions for proactively addressing alarms and alerts. For example, you shall be able to create multiple customized lists of “allow” license plates that are associated with executives, VIPs, etc. These plates shall generate an alert upon entry, and stakeholders shall be immediately notified and provided with a list of to-dos, like unlock certain doors, turn on lights, etc. Similarly, license plates on the “block” list shall have unique procedures that you can easily follow for threat mitigation.
c.	Bullet Camera Version
1)	The IP bullet camera shall incorporate a camera/lens combination and embedded License Plate Recognition (LPR) technology; the license shall be included. The bullet camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera shall be available in 8 MP resolution model and shall have true WDR and Smart IR/Adaptive capability; includes an integral 3.6-10 mm or 8-18 mm lens varifocal DC-iris lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 131 ft (40 m) with 4 IR LEDs. 
2)	The bullet camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and rotation (roll), for any angle of view required. A variety of mounting options shall be available. 
3)	The bullet camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting. 
4)	The bullet camera shall be powered by PoE+, 24 VAC or 12 VDC. A dual heater system shall be provided; It maintains proper temperature in the camera housing and prevents fogging of the window. For low temperature operation: heater turns on at -40° F (-40° C) and off at 59° F (15° C). For defog operation: heater turns on at -40° F (-40° C) and off at 140° F (60° C.
5)	The bullet camera shall have triple streaming video and support H.264/H.265 and M-JPEG image compression. The camera shall also have smart encoding to further improve video encoding and storage capacity.
6)	The bullet camera features shall include motorized autoiris, Automatic Gain Control (AGC), True Wide Dynamic Range (TWDR), white balance, defog, flip, mirror, privacy masking, Dynamic Region of Interest (ROI), Backlight Compensation (BLC) / Highlight Compensation (HLC) and motion detection.
7)	The bullet camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance, including front glass. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.
8)	The bullet camera shall include a slot for an SD card for local storage. 32 GB SD card shall be provided. If other SD card is used its requirements are: Class 10; read speed: 100 MB/sec; write speed: 60 MB/sec.
9)	The bullet camera shall meet or exceed the following design and performance specifications.

a.	Imaging Device:		1/1.8-inch progressive scan
b.	Max. Resolution:		3840 x 2160 (8 MP) 
c.	Shutter Speed:		Auto (1/2 - 1/10,000 sec), 
                                             manual
d.	Automatic Gain Control:	On/Off selectable
e.	Minimum Illumination	Color: 3.6-10mm: 0.02 lux or 
                                              8-18 mm: 0.01 lux;
                                              B&W: 0.01 lux/ 0 lux (IR Off/On)
f.	Tilt and Horizontal		Three-direction adjustment, 
                                              allowing for adjustment of pan, 
                                              tilt and rotation (roll)
g.	Digital Zoom:		Yes (DROI)
h.	Lens Adjustment:		Motorized lens, P-iris 
                                             automatically adjusts to zoom 
                                             condition
i.	Focal Length:		3.6-10 mm; 2.8X optical zoom 
                                             or 8-18 mm, 2.25X optical zoom
j.	Horizontal Field of View:	3.6-10 mm: 98°- 46° (wide-tele) 
                                             or 
                                             8-18 mm: 60°- 25° (wide-tele)
k.	Vertical Field of View:	3.6-10 mm: 54°- 26° (wide-tele) 
                                             or
                                             8-18 mm: 33°- 12° (wide-tele)
l.	IR Distance:		Smart IR/Adaptive IR; 131 ft 
                                             (40 m) with 4 IR LEDs
m.	Dual Heater System:	For low temperature operation: 
                                             heater turns on at -40° F
                                             (-40° C) and off at 59° F (15° C). 
                                             For defog operation: heater 
                                             turns on at 40° F and off at 
                                             140° F (60° C).
  Electrical Specifications
a.	Input Voltage:		24 VAC, 12 VDC or PoE+
b.	Current:		PoE: 0.41 A; 24 VAC: 0.82 A; 
                                                   12 VDC: 1.64 A 
c.	Power Consumption:	IR/Heaters On: 19.68 W; 
                                                    IR Off/Heaters On: 12.48 W
d.	Connectors:		Pigtail cable provided; optional 
                                                    backbox required for cabling
                                                    Power: 12 VDC or 24 VAC 
                                                    terminal block
                                                    PoE: RJ-45
                                                    Video/Data: RJ-45
                                                    Alarm: screw terminal
                                                    Audio: screw terminal; audio 
                                                    level alarm alert
                                                    Slot for SD card (supplied)
                                                    Reset button
                                                    Default button
e.	Radio Frequency
             Emission Rating: 	FCC Class A; CE

                                                             Environmental Specifications
a.	Operating Temperature:	-40° to 140°F (-40° to 60°C)
b.	Humidity:		Up to 90% relative, non-condensing
                                                            Physical Specifications
a.	Construction:		Aluminum alloy body; 
                                                                                    sunshield: PC+ABS
b.	Dimensions:		Length: 10.3 in. (261 mm), 
Diameter: 		3.5 in. (89 mm)
c.	Weight: 		4 lb (1.8 kg)
                                                         Mechanical Specifications
a.	Camera Mount:		Surface mount 
b.	Adjustments:		3-axis camera adjustment: 
                                                   pan 360°; tilt 0°-90°; roll 360° 
d.	Box Camera Kit Version
1)	The LPR box camera kit shall be lightweight and compact and shall include embedded License Plate Recognition (LPR) technology; the license shall be included. The kit shall include the camera, a lens, a housing and a wall mount. The high-resolution day/night camera shall be available in 8 MP resolution and shall have true WDR. Day/night operation shall be achieved using a built-in IR-cut filter.
2)	The box camera shall have triple streaming video and support H.264/H.265 and M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.
3)	The box camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, BLC/HLC and motion detection.
4)	The box camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.
5)	The box camera shall provide a slot for an SD card for local storage which shall be provided.
6)	The box camera shall meet or exceed the following design and performance specifications.
7)	Camera Parameters:
a)	Imaging Device:  1/1.8 inch progressive scan.
b)	Maximum Resolution:  8 MP.
c)	Shutter Speed:  1/2 - 1/10,000 sec.
d)	Automatic Gain Control:  On/Off selectable.
e)	Sensitivity:  Color:  0.02 lux. Black and White:  0.01 lux. 
f)	Adjustment, Tilt and Horizontal:  Dependent on mount
g)	Digital Zoom:  Dynamic ROI.
8)	Physical Parameters:
a)	Operating Temperature:  14 to 131 degrees F (minus 10 to 55 degrees C).
b)	Construction:  Aluminum and plastic.
c)	Dimensions, H x W x L:  2.4 in (62 mm) x 2.9 in (73 mm) x 4.1 in (104 mm).
d)	Weight:  Approximately 1.3 lbs (0.8 kg).
9)	Electrical Parameters:
a)	Input Voltage:  PoE; 24 VAC, 12 VDC. 
b)	Current:  PoE:  0.28 A; 12 VDC:  1.125 A; 24 VAC:  0.56 A.
c)	Power Consumption:  13.5 W.
d)	Connectors:
1)	Power:  24 VAC/12 VDC terminal block.
2)	PoE:  RJ-45.
3)	Video/Data:  RJ-45.
4)	Audio Input/Output:  terminal block; audio level alarm alert.
5)	Slot for SD card.
6)	Reset button.
7)	Default button.
e)	Radio Frequency Emission Rating:  FCC Class A; CE.
e.	Box Camera/Housing Kit Version -
1)	The LPR box camera shall be lightweight and compact and shall include embedded License Plate Recognition (LPR) technology; the license shall be included. The kit shall include a 9-50 varifocal lens, outdoor housing, wall mount and IR illuminator. The high-resolution day/night camera shall be available in 8 MP resolution and shall have true WDR. Day/night operation shall be achieved using a built-in IR-cut filter.
2)	Refer to above for Box Camera specifications and features.
3)	Camera Housing specifications.
a.	Electrical Specifications
1)	Power Input: 60 W/90 W PoE IEEE 802.bt; 50-57 VDC
2)	Power Consumption (PoE): 37.5 W. Camera: 13.5 W; De-Icing Window: 10 W; Fan: 2 W; IR Illuminator: 12 W.
3)	Deicing Window Heater: On:  68 degrees F (20 degrees C) or less. Off:  86 degrees F (30 degrees C) or greater. 10 W.
4)	Fan:  On:  95 degrees F (35 degrees C) or greater. Off:  77 degrees F (25 degrees C) or less. 2 W
5)	Integral IR LEDs: 21 W; 164-459 ft (50-140 m) range
b.	Environmental Specifications
1)	Operating Temperature: -4° to 149°F (-20° to 65°C); -4° to 122°F (-20° to 50°C) with IR LEDs.
c.	Physical Specifications
1)	Construction: Cast aluminum alloy
2)	Viewing Window: Chemically strengthened glass
3)	Coating: White epoxy powder
4)	External Dimensions: 9.52 x 19.8 inches (241.7 x 502.8 mm)
5)	Internal Dimensions: 4.13 x 3.05 x 10.03 inches. (105 x 77.4 x 255 mm)
6)	Weight: 13 lb (5.9 kg)
4)	Lens Specification
a.	Lens: 	1/1.8” format; CS mount; 9-50 focal length; 
                      field-of-view (16:9): 46.1º x 26.3 º 
b.	IR Distance: From housing: 164-459 ft (50-140 m) range
11)	LPR Specification
a.	Region of Interest:	Provides calibration pattern for easy setup
b.	Lists: 			Standard allowlist/blocklist and custom lists; 50 user-
                                       defined lists including 4 pre-defined lists; list 
                                       synchronization between cameras on the system. 
                                       Schedules and rules management for each list.
                                       10,000 max plates per list.
c.	Event Responses: 	Vicon VMS Valerus, alarm out and FTP
d.	Event Logs: 		Search capabilities with captured image and plate 
                                       thumbnail
e.	Storage Options: 	Customizable
f.	Number of Events on 
SD Card: 		Up to 800,000 events on 32 GB card supplied 
                                       (25,000 events/GB)
g.	Recognition Rate: 	95%-99%, depending on country and installation 
                                       conditions
h.	Direction Detection: 	Yes
i.	Installation Parameters: 	Vehicle Speed: 15 mph (20 km/hr) max
                                       Detection Time: 100-1000 ma
                                       Character Height: Pixels:13 min; 25 recommended
                                       Target Distance: Bullet: 3.6-10 mm lens: 6.6-19.7 ft (2-6 m); 
                                       8-18 mm lens: 16-36 ft (5-11 m). Box Kit: 16-100.7 ft (5-30.48 m)
                                       Maximum Horizontal/Vertical Angle: 35º max; 20º 
                                       recommended/35º max; 20º recommended
                                       Lane Coverage: Two max; 1 recommended
                                       Application: Vehicle entry/exit
12)	Network Video Specifications
a.	Communication Platform:	Open platform; compatible with Valerus 
	             Video Management System 
b.	Compression:	             Smart Encoding; H.264/H.265; M-JPEG 
c.	LAN Interface:	            10 Base-T/100 Base-TX, Unicast/Multicast
d.	Video Channels	            Triple streaming
e.	Resolution and Frame Rate:	8 MP: 3840x2160, 3264x1840, 2592x1944, 2688x1520, 
                                                    2048x1536, 1920x1080, 1280x960/720, 800x600, 
                                                    640x480, 640x360, 320x240
                                                                       Max 30 fps 
F.	Web Browser:		Safari, Firefox, Chrome, Microsoft 
                                                          Edge
G.	Users:		Live viewing for up to 10 clients
H.	Image Settings:		Digital image effects defog, flip and mirror; configurable 
                                                          brightness, contrast, saturation, hue, sharpness; BLC; 
                                                          HLC; gamma correction; 3 DNR; motion detection; 
	             white balance, AGC; Electronic Shutter, automatic or 
	             manual; digital zoom; motion detection; privacy masks;
                                                          motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:		Tampering/Defocus, Intelligent Motion Detection 
                                                           Intrusion Detection; Line Counting/Cross, Loitering, 
                                                          Object Left/Removed, Wrong Direction, Area Counting
J.	Supported Protocols:		IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                                          RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, 
                                                          HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, 
                                                          DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                                         S/G/Q/T
C.	Pan-Tilt-Zoom (PTZ) Cameras:
1.	Basis of Design:  V2002D-PTZ and V2005D-PTZ, Outdoor IP PTZ Network Compact Dome Cameras as manufactured and supplied by Vicon Industries.
a.	Certifications:  CE, UL, FCC, Class A, IP67, IK07, ONVIF S/T/G/M, RoHS and NDAA/GSA/TSA compliant.
b.	General Features:
1)	Equipment and Materials:  Standard components regularly manufactured and used in manufacturer’s system.
2)	Systems and Components:  Tested and proven in actual use.
3)	Technical Support:  Toll free 24-hour phone number from manufacturer. No charge service for dealers and installers.
4)	Provided with an explicit 5-year manufacturer warranty.
5)	Camera, lens, and pan/tilt drive in covert dome enclosure.
a)	Resolution:  V2002D-PTZ: 2 MP with true WDR; V2005D-PTZ: 5 MP with true WDR.
b)	Lens:  Integral varifocal 4.5-135 mm (2 MP version); 5.2-148 mm (5 MP version); 30X optical zoom, 8X digital zoom.
c)	Day/night Operation:  Built-in IR-cut filter.
d)	Starlight low-light imaging.
e)	IR Distance:492 ft (150 m).
f)	Automatic Smart IR/Adaptive IR capability.
6)	Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross/counting, loitering, object left/removed, wrong direction and area counting. The 5 MP model shall also provide AI-based object classification analytics for vehicles, people, and animals. This shall enhance working with Museum Search in Valerus VMS.
7)	Powered By:  PoE++, 24 VAC, or 48 VDC.
8)	Heater/Blower System:  Maintains proper temperature in camera housing and prevents window fogging.
9)	Triple Streaming Video and Network Video Transmission:  using either H.264/H.265 and M-JPEG compression.
a)	Smart Encoding:  Further improves video encoding and improves storage capacity.
b)	Transmits high quality video across network for remote viewing and recording.
c)	Configurable remotely from network digital video recorders and master workstations.
10)	Two Alarm Inputs:  Programmable for functional state (enabled or disabled); set to Normally Open (NO) or Normally Closed (NC).
11)	Alarm Outputs:  Control external equipment and may be set for Normally Open (NO) or Normally Closed (NC).
12)	An audio alert is available.
13)	Individual Programmable Preset Positions:  128. Each able to be titled and adjustable for pan and tilt speed and manual or auto focus.
14)	Four Tours (Patrols):  Available with 128 presets per tour. Each tour able to be titled and adjustable for pan, tilt, zoom speed, and dwell time. Programmed to repeat.
15)	Pan and Tilt Functions:  Programmable.
a)	Maximum Manual Pan and Tilt Speeds:  Programmable.
b)	Maximum Pan Speed:  300 degrees per sec.
c)	Maximum Tilt Speed:  160 degrees per sec.
d)	Pan and Tilt Speeds:  Scalable to zoom setting.
e)	Pan Range:  360 degree continuous.
f)	Tilt Range:  195 degrees (minus15 to 90 degrees).
16)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
17)	Meets FCC requirements for Class A device.
a)	Supports industry-standard ONVIF S/T/G/M interface.
b)	IP67-rated to withstand rain, dust, and vandalism.
c)	IK7 rated for impact resistance.
d)	Meets latest regulations required to be NDAA, GSA schedule and TAA approved.
18)	Provide a slot for an SD card for local storage.
c.	Day/Night IP Dome Camera Specifications:
1)	Imaging Device:  1/2.8 inch progressive scan.
2)	Maximum Resolution:  2 MP or 5 MP.
3)	Shutter Speed:  1/30 to 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	WDR:  True WDR (120 dB).
6)	Sensitivity (at 30 IRE):  V2002D-PTZ:  Color:  0.007 lux; B and W:  0.002 lux. V2005D-PTZ: Color:  0.03 lux; B and W:  0.01 lux.
7)	Pan/Tilt Range:  360 degree continuous pan; 95 degree tilt (minus 15 to 90 degree).
8)	Lens:  
a)	V2002D-PTZ:  4.5 to 135 mm, 30X optical zoom.
b)	V2005D-PTZ: 5.2 to 148 mm, 30X optical zoom
9)	Digital Zoom:  8X.
10)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition (manual mode).
11)	Horizontal Field of View:  V2002D-PTZ: 60 - 5 degrees (wide-tele). V2005D-PTZ: 58.1 to 2.14 degrees (wide-tele).
12)	Vertical Field of View:  V2002D-PTZ: 38-3 degrees (wide-tele). V2005D-PTZ: 33.8 to 1.2 degrees (wide-tele).
13)	IR Distance:  492 ft (150 m); Smart IR/Adaptive IR automatic IR 
14)	Heater/Blower System:  For low temperature operation. Heater turns on at 59 degrees F (15 degrees C); blower is always on.
d.	Electrical Specifications:
1)	Input Voltage:  24 VAC plus 20 or minus 10 percent, 48 VDC plus or minus 10 percent or PoE++.
2)	Current:  24 VAC:  2.5 A; 48 VDC:  1.25 A.
3)	Power Consumption:  Total 48 W. PTZ Camera 11 W; Pan/Tilt Function: 12 W;  IR:  19 W; Heater:  5.5 W; Blower:  0.9 W.
4)	Connectors:  Power: 48 VDC or 24 VAC terminal block; PoE:  RJ-45.
a)	Video/Data:  RJ-45.
b)	Alarm:  Screw terminal.
c)	Audio:  Screw terminal.
d)	Slot for SD card (128 G max customer supplied card).
e)	Reset button.
f)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
e.	Environmental Specifications:
1)	Operating Temperature:  Minus 40 to 140 degrees F (Minus 40 to 60 degrees C).
2)	Humidity:  Up to 90 percent relative, non-condensing.
f.	Physical Specifications:
1)	Construction:  Aluminum base; polycarbonate clear dome.
2)	Dimensions:  Height: 13.2 inches (336 mm).
3)	Diameter:  7.5 inches (190 mm).
4)	Weight:  11.5 lbs (5.2 kg).
g.	Mechanical Specifications:
1)	Camera Mount:  Mounting accessories available.
2)	Adjustments:  Pan 360 degrees continuous; tilt: 95 degrees (-15 degrees -90).
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution and Frame Rate:  2 MP: 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240. 5 MP: 2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x108 Max 30 fps.
6)	Web Browser:  Safari, Firefox, Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF, S/G/M/T.
i.	Warranty:  5 years, parts, and labor. 
2.	Basis of Design:  V2008PTZ-IR, Outdoor IP PTZ Network Compact Dome Cameras as manufactured and supplied by Vicon Industries.
a.	Certifications:  CE, UL (pending), FCC, Class A, IP66, IK10, ONVIF S/T/G, RoHS and NDAA/GSA/TSA compliant.
b.	General Features:
1)	Equipment and Materials:  Standard components regularly manufactured and used in manufacturer’s system.
2)	Systems and Components:  Tested and proven in actual use.
3)	Technical Support:  Toll free 24-hour phone number from manufacturer. No charge service for dealers and installers.
4)	Provided with an explicit 5-year manufacturer warranty.
5)	Camera, lens, and pan/tilt drive in covert dome enclosure.
a)	Resolution:  8 MP with true WDR.
b)	Lens:  Integral varifocal 6.5-230 mm; 35X optical zoom, 8X digital zoom.
c)	Day/night Operation:  Built-in IR-cut filter.
d)	Starlight low-light imaging.
e)	IR Distance:1312 ft (400 m).
f)	Adaptive IR capability.
6)	Intelligent Video Analysis: tampering, motion detection and auto-tracking (people); supports Museum Search.
7)	Powered by:  PoE++ or 24 VAC.
8)	Triple Streaming Video and Network Video Transmission:  using either H.264/H.265 and M-JPEG compression.
a)	Smart Encoding:  Further improves video encoding and improves storage capacity.
b)	Transmits high quality video across network for remote viewing and recording.
c)	Configurable remotely from network digital video recorders and master workstations.
9)	One Alarm Input:  Programmable for functional state (enabled or disabled); set to Normally Open (NO) or Normally Closed (NC).
10)	Alarm Output:  Control external equipment and may be set for Normally Open (NO) or Normally Closed (NC).
11)	Individual Programmable Preset Positions:  256. Each able to be titled and adjustable for pan and tilt speed and manual or auto focus.
12)	Eight Tours:  Available with 32 presets per tour. Each tour able to be titled and adjustable for pan, tilt, zoom speed, and dwell time. Programmed to repeat.
13)	Pan and Tilt Functions:  Programmable.
a)	Maximum Manual Pan and Tilt Speeds:  Programmable.
b)	Maximum Pan Speed:  720 degrees per sec.
c)	Maximum Tilt Speed:  540 degrees per sec.
d)	Pan and Tilt Speeds:  Scalable to zoom setting.
e)	Pan Range:  360 degree continuous.
f)	Tilt Range:  Minus 20 to 90 degrees.
14)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
15)	Meets FCC requirements for Class A device.
a)	Supports industry-standard ONVIF S/T/G interface.
b)	IP66-rated to withstand rain, dust, and vandalism.
c)	IK10 rated for impact resistance.
d)	Meets latest regulations required to be NDAA, GSA schedule and TAA approved.
16)	Provide a slot for an SD card for local storage.
c.	Day/Night IP Dome Camera Specifications:
1)	Imaging Device:  1/1.8 inch progressive scan.
2)	Maximum Resolution:  8 MP.
3)	Shutter Speed:  1/7 to 1/16,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	WDR:  True WDR (130 dB).
6)	Sensitivity (at 30 IRE):  Color:  0.04 lux; B and W:  0.01 lux (IR Off; 
0 lux, IR On.
7)	Pan/Tilt Range:  360 degree continuous pan; minus 20 to 90 degree tilt.
8)	Lens:  
a)	6.5 to 230 mm, 35X optical zoom.
9)	Digital Zoom:  8X.
10)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition (manual mode).
11)	Horizontal Field of View:  60.4 to 2.0 degrees (wide-tele).
12)	Vertical Field of View:  35.9 to 1.2 degrees (wide-tele).
13)	IR Distance:  1312 ft (400 m); Adaptive IR automatic IR 
d.	Electrical Specifications:
1)	Input Voltage:  24 VAC (+20%/-10%) or PoE++ 
(IEEE 802.3bt, Class 8).
2)	Current:  24 VAC:  3.25 A.
3)	Power Consumption:  Total 71 W.
4)	Connectors:  Power: 24 VAC terminal block; PoE:  RJ-45.
a)	Video/Data:  RJ-45.
b)	Alarm:  Screw terminal.
c)	Audio:  Screw terminal.
d)	Slot for SD card (1 TB max customer supplied card).
e)	Reset button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
e.	Environmental Specifications:
1)	Operating Temperature:  Minus 40 to 149 degrees F (Minus 40 to 65 degrees C).
2)	Humidity:  10 to 90 percent relative, non-condensing.
f.	Physical Specifications:
1)	Construction:  Aluminum sunshield/housing; coated glass lens cover.
2)	Dimensions:  Height: 14.2 inches (361.9 mm).
3)	Diameter:  7.5 inches (190 mm).
4)	Weight:  11 lbs (5 kg).
g.	Mechanical Specifications:
1)	Camera Mount:  Mounting accessories available.
2)	Adjustments:  Pan 360 degrees continuous; tilt: minus 20 degrees - 90).
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10/100/1000 Base-T, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution and Frame Rate:  3840x2160, 2560x1440, 1920x1080, 1280x960/720, 720x408, 640x360. Max 30 fps.
6)	Web Browser:  Safari, Firefox, Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks (32); OIS; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Tampering, Motion Detection, Auto-Tracking (people); Museum Search.
10)	Supported Protocols:  IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, SSL, Bonjour, Firewall, 802.1x, ONVIF S/G/M/T.
i.	Warranty:  5 years, parts, and labor. 
D.	Box Cameras:
1.	Basis of Design:  V2008-W-NL IP Box Camera as manufactured and supplied by Vicon Industries:
a.	Certifications:  CE, UL, FCC Class A, ONVIF S/T/G/Q, RoHS, NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Mounting:  1/4-20 mounting holes, top and bottom. 
2)	Lens:  DC iris.
3)	Lens:  P-iris.
4)	Lens:  i-CS.
5)	Day/night Operation:  Built-in IR-cut filter. 
6)	Wide Dynamic Range (WDR):  8 MP.
7)	Triple streaming video. 
8)	Camera features:  Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, and motion detection.
e.	Camera Parameters:
1)	Imaging Device:  1/1.8 inch progressive scan.
2)	Maximum Resolution:  8 MP.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.02 lux. Black and White:  0.01 lux. 
6)	Adjustment, Tilt and Horizontal:  Dependent on mount
7)	Digital Zoom:  Dynamic ROI.
f.	Physical Parameters:
1)	Operating Temperature:  14 to 131 degrees F (minus 10 to 55 degrees C).
2)	Construction:  Aluminum and plastic.
3)	Dimensions, H x W x L:  2.4 in (62 mm) x 2.9 in (73 mm) x 4.1 in (104 mm).
4)	Weight:  Approximately 1.3 lbs (0.8 kg).
g.	Electrical Parameters:
1)	Input Voltage:  PoE; 24 VAC, 12 VDC. 
2)	Current:  PoE:  0.350 mA; 12 VDC:  1 A; 24 VAC:  1 A (50/60 Hz).
3)	Power Consumption:  13.5 W.
4)	Connectors:
a)	Power:  24 VAC/12 VDC terminal block.
b)	PoE:  RJ-45.
c)	Video/Data:  RJ-45.
d)	Audio Input/Output:  terminal block; audio level alarm alert.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Platforms:
1)	Communication Platform:  Open platform.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
6)	Frame Rate:  Maximum 30 fps.
7)	Web Browser:  Firefox, Chrome, Safari, or Microsoft Edge.
8)	Users:  10 user live viewing.
9)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; dynamic ROI.
10)	Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals. This shall 
enhance working with Museum Search in Valerus VMS.
11)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/M/T.
E.	Specialty Cameras:
1.	Basis of Design:  V-CELL-HD-C Corner Mounted HD Day/Night Camera as manufactured by Vicon Industries: Additionally, a camera module, V-CELL-HD-CMOD, shall be available to retrofit any existing V-CELL camera to 5 MP.
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, NDAA-compliant
b.	Features:
1)	Ideal for custodial suites and prison cells.
2)	Mounting:  Stainless steel, waterproof housing. Fits into 90 degree corners. Fixed mounting frame and removable front plate. Assembly is permanently sealed to walls and ceiling making housing ligature proof. Front plate is recessed and secured to fixed frame with security screws. Two windows in front plate protect camera and IR LED illuminators. 
3)	Camera Mount:  Adjustable allowing for tilting up or down for an exact view.
4)	Alarms and audio. 
5)	Privacy masks.
c.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan RGB CMOS.
2)	Camera Type:  True day/night (IR cut filter)
3)	Sensitivity:  Color:  0.003 lux. B&W:  0.001 lux (IR Off); 0.0 lux (IR On)
4)	IR Distance:  98 ft (30 m) Smart IR On/Off.
5)	Lens Focal Length:  2.4 mm, fixed wide angle.
6)	Aperture:  f/2.1 maximum.
7)	Horizontal Field of View:  121 degrees.
8)	Vertical Field-of-View:  93 degrees.
d.	Physical Parameters:  
1)	Operating Temperature:  -4 to 140 degrees F -20 (0 to 60 degrees C).
2)	Application:  Indoor.
3)	Construction:  Enclosure:  Stainless steel; brushed satin. Mounting Frame:  14 gauge; camera mount:  14 gauge. Windows:  polycarbonate. IR:  5 mm thick. Camera:  6 mm thick. Dimensions:  15 in. (380 mm) x 12.6 in. (320 mm).
4)	Weight:  3.3 lbs (1.5 kg) approximate. 
e.	Electrical Parameters:  
1)	Input Voltage:  24 VAC. 12 VDC. PoE +.
2)	Power Consumption:  Approximately 12.95 (IR on); 7.85 (IR Off).
3)	Connectors, 24 VAC and 12 VDC:  Screw terminal.
4)	Connectors, PoE:  RJ-45.
5)	Connectors, Alarms (In/Out) and Audio (mic/spkr):  Screw terminal. 
6)	Radio Frequency Emission Rating:  FCC Class A.
f.	Network Parameters:
1)	Compression:  H.264, MPEG-4 or M-JPEG and analog.
2)	Video Streams:  10 concurrent.
3)	Video Resolution:  2592x1944 (5 MP), 2688x1520, 2048x1536 (3 MP), 1920x1080 (Full HD 1080P), 1280x1024 (SXVGA), 1280x720 (HD 720P), 704x480/576 (D1), 640x480 (VGA), 352x240/288 (CIF), 320x240 (QVGA).
4)	Frame Rate:  Up to 30 fps (5 MP).
5)	Video Bandwidth:  10/100 Mbps.
6)	    Streaming: Triple
7)	    Image Settings: Digital image effects defog, flip and mirror;   
    configurable brightness, contrast, saturation, hue, sharpness; BLC; 
    HLC; gamma correction; 3 DNR; motion detection; white balance, 
    AGC; Electronic Shutter, automatic or manual; digital zoom; motion 
    detection; privacy masks; dynamic ROI
8)	    Intelligent Video Analytics:  Tampering, Intelligent Motion Detection 
    Intrusion Detection; Line Cross, Loitering, Object Left/Removed, 
    Tailgating, Crowding. It shall also provide AI-based object 
    classification analytics for vehicles, people, and animals. This shall 
    enhance working with Museum Search in Valerus VMS.
9)	    Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, 
    RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, 
    ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, 
    PPPoE, Bonjour, ONVIF S/G/M/T.

2.	Basis of Design:  V2005CNR-W24IR Corner Mounted HD Day/Night Camera as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, NDAA-compliant
b.	Features:
1)	Ideal for environments where there is risk of tampering or destruction.
2)	Mounting:  Fits into 90 degree corners. Fixed mounting frame and removable front plate; once installed into the corner, the housing shall be ligature proof. Front plate is secured to fixed frame with security screws. The front plate shall have two windows to protect the camera and IR LED illuminators. 
3)	Camera Mount:  Adjustable allowing for tilting up or down for an exact view.
4)	Alarms and audio. 
5)	Privacy masks.
c.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan RGB CMOS.
2)	Camera Type:  True day/night (IR cut filter).
3)	Sensitivity:  Color:  0.003 lux. B&W:  0.001 lux (IR Off); 0.0 lux (IR On).
4)	IR Distance:  98 ft (30 m) Smart IR On/Off.
5)	Lens Focal Length:  2.4 mm, fixed wide angle.
6)	Aperture:  f/2.1 maximum.
7)	Horizontal Field of View:  121 degrees.
8)	Vertical Field-of-View:  93 degrees.
d.	Physical Parameters:  
1)	Operating Temperature:  -4 to 140 degrees F -20 (0 to 60 degrees C).
2)	Application:  Indoor.
3)	Construction:  Enclosure:  Aluminum. Windows:  polycarbonate. IR:  5 mm thick. Camera:  6 mm thick.
4)	Weight:  4.4 lbs (2 kg) approximate. 
e.	Electrical Parameters:  
1)	Input Voltage:  24 VAC. 12 VDC. PoE +.
2)	Power Consumption:  Approximately 12.9 (IR on); 7.85 (IR Off).
3)	Connectors, 24 VAC and 12 VDC:  Screw terminal.
4)	Connectors, PoE:  RJ-45.
5)	Connectors, Alarms (In/Out) and Audio (mic/spkr):  Screw terminal. 
6)	Radio Frequency Emission Rating:  FCC Class A.
f.	Network Parameters:
1)	Compression:  H.264, MPEG-4 or M-JPEG and analog.
2)	Video Streams:  10 concurrent.
3)	Video Resolution:  2592x1944 (5 MP), 2688x1520, 2048x1536 (3 MP), 1920x1080 (Full HD 1080P), 1280x1024 (SXVGA), 1280x720 (HD 720P), 704x480/576 (D1), 640x480 (VGA), 352x240/288 (CIF), 320x240 (QVGA).
4)	Frame Rate:  Up to 30 fps (5 MP).
5)	Video Bandwidth:  10/100 Mbps. Streaming: Triple
6)	    Image Settings: Digital image effects defog, flip and mirror;   
    configurable brightness, contrast, saturation, hue, sharpness; BLC; 
    HLC; gamma correction; 3 DNR; motion detection; white balance, 
    AGC; Electronic Shutter, automatic or manual; digital zoom; motion 
    detection; privacy masks; dynamic ROI
7)	    Intelligent Video Analytics:  Tampering, Intelligent Motion Detection 
    Intrusion Detection; Line Cross, Loitering, Object Left/Removed, 
    Tailgating, Crowding. It shall also provide AI-based object 
    classification analytics for vehicles, people, and animals. This shall 
    enhance working with Museum Search in Valerus VMS.
8)	    Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, 
    RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, 
    ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, 
    PPPoE, Bonjour, ONVIF S/G/M/T.

F.	Dome Cameras:
1.	Basis of Design:  V2020-WIR-360/V2032-WIR-360 Multi-Sensor Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, ONVIF S/G/ M /T and NDAA/GSA/TAA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Outdoor multi-sensor camera incorporating four camera or lens modules for a 180, 270, or 360 degree panoramic view.
2)	True WDR and IR capability with four integral motorized lenses.
3)	Electronic iris, AGC, white balance, backlight compensation, tampering, flip, mirror, privacy masks and motion detection.
4)	Mounting:  Surface mountable. Wall, corner and pole mounting accessories available. 
e.	Camera Parameters:
1)	Imaging Device:  5 MP:  4x 1/2.8-inch progressive scan CMOS.
                            8 MP: 4x 1/1.8-inch progressive scan CMOS Starlight.
2)	Maximum Resolution:  4x 2592 x 1944, 5 MP; 4x 3840 x 2160, 8 MP.
3)	Shutter Speed:  1/7 - 1/20,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity @30 IRE:  5 MP: Color:  0.03 lux; B&W:  0.01 (IR OFF), 0 lux (IR On). 8 MP: Color:  0.02 lux; B&W:  0.01 (IR OFF), 0 lux (IR On).
6)	Wide Dynamic Range:  True WDR, 120dB.
7)	Lens Focal Length:  5 MP: 4x 3.1-10 mm; 8 MP: 4x 3.6-10 mm.
8)	Horizontal Field of View:  5 MP: 32 to 96 degrees; 
8 MP: 46 to 98 degrees.
9)	Vertical Field-of-View:  5 MP: 24 to 69 degrees; 8 MP: 26 to 54 degrees.
10)	Field-of-View Depth:  5 MP: 40 to 124 degrees; 8 MP: 54 to 113 degrees.
11)	IR Distance:  Up to 131 feet (40 m). 
f.	Physical Parameters:  
1)	Operating Temperature:  -40 to 131 degrees F (-40 to 55 degrees C).
2)	Operating Humidity:  10 to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Enclosure:  Die-cast aluminum housing. Dome:  Clear polycarbonate. Dimensions:  5.6 in. (142.3 mm) x 9.7 in. (247.5 mm) diameter.
5)	Weight:  5.2 lbs (2.36 kg) approximate. 
g.	Electrical Parameters:  
1)	Input Voltage/Current:  PoE++ (IEEE802.3bt), 24 VAC, 24 VDC. 1.7 A.
2)	Power Consumption (IR on):  40 W.
3)	Connectors:  Pigtail:  Power:  terminal block.
4)	Connectors, PoE:  RJ-45.
5)	Connectors, Alarms (In/Out):  Terminal block. 
6)	Connectors, Audio:  Phone jack. 
7)	Connectors:  Slot for SD card. 
8)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus and ViconNet Video Management Systems
2)	Compression:  H.264/H.265.
3)	LAN Interface:  Triple streaming.
4)	Video Resolution:  4x 2592x1944.
5)	Frame Rate:  Up to 30 fps.
6)	Web Browser:  Firefox, Google Chrome.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Day/night mode; flip and mirror; configurable brightness, contrast, hue, sharpness, saturation; white balance, gain control; DNR; true WDR (120dB); privacy masks (5); motion detection; BLC; Exposure; Audio.
9)	Video Content Analytics:  Video Contents Analysis:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
10)	Supported Protocols:  IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTP, RTCP SMTP, FTP, UDP, uPnP, QoS, ICMP, SNMP v2c/v3, SSL, DNS, NTP, LDAP (client), Zeroconfig, DynDNS, ONVIF S/G/M/T.
2.	Basis of Design:  V2005D Outdoor IP Micro Dome Camera with built in Mic as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, ONVIF S/G/M/T and NDAA/GSA/TAA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Outdoor fixed dome camera shall incorporate a fixed camera/lens combination.
2)	The camera shall have bi-directional audio, built-in mic and line out.
3)	True WDR and Smart or Adaptive IR capability.
4)	Intelligent Video Analysis, tampering, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting.
5)	Mounting:  Surface mountable. 
e.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan.
2)	Maximum Resolution:  5 MP.
a)	Sensitivity:  Color:  0.03 lux; Black and White:  0.01 (IR OFF), 0 lux (IR On).
b)	Horizontal Field of View:  104 degrees.
c)	Vertical Field-of-View:  78 degrees.
d)	Field-of-View Depth:  134 degrees.
e)	Resolution:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Digital Zoom:  Yes, ROI.
6)	Lens Adjustment:  Fixed.
7)	Lens Focal Length:  2.8 mm.
8)	IR Distance:  Smart IR/Adaptive IR; 49 ft (15 m) with 8 IR LEDs.
f.	Physical Parameters:  
1)	Operating Temperature:  Minus 22 to 131 degrees F (Minus 30 to 55 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum dome housing; polycarbonate clear dome. Dimensions:  2.2 in. (57 mm) x 4.3 in. (110 mm) diameter.
5)	Weight:  1.65 lbs (0.75 kg). 
g.	Electrical Parameters:  
1)	Input Voltage/Current:  PoE, 0.28A.
2)	Power Consumption, IR on: 9 W; IR off: 6.6 W.
3)	Connectors:  
a)	Pigtail cable.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Audio:  Built-in Mic/Audio Output: screw terminal block. 
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
4)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Frame Rate:  Up to 30 fps.
5)	Web Browser:  Safari, Firefox, Google Chrome, Microsoft Edge.
6)	Users:  Live viewing for up to 10 clients.
7)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
8)	Intelligent Video Analytics:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. The camera shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
9)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/M/T.
3.	Basis of Design:  V2000D Outdoor IP Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/M/T and NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Outdoor fixed dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart or Adaptive IR capability.
3)	Intelligent Video Analysis, tampering, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting.
4)	Mounting:  Surface mountable. 
e.	Camera Parameters:
1)	Maximum Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  3.1 to 10 mm: 0.03 lux or 8 to 18 mm: 0.02 lux; 
Black and White:  0.01 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  3.1 to 10 mm: 96 to 32 degrees or 
8 to 18 mm: 40 to 17 degrees.
d)	Vertical Field-of-View:  3.1 to 10 mm: 69 to 24 degrees or 
8 to 18 mm: 29 to 13 degrees.
e)	Resolution:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
f)	Lens Focal Length:  3.1 to 10 mm varifocal or 8-18 mm varifocal.
g)	Current:  PoE:  0.3 A; 24 VAC:  0.6 A; 12 VDC:  1.2 A.
h)	Power Consumption IR and Heaters On:  16.5 W.
2)	Maximum Resolution:  8 MP.
a)	Imaging Device:  1/1.8-inch progressive scan.
b)	Sensitivity:  Color:  3.6 to 10 mm: 0.02 lux or 8 to 18 mm: 0.01 lux; 
Black and White:  0.01 lux (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  3.6 to 10 mm: 96 to 46 degrees or 
8 to 18 mm: 104 to 48 degrees.
d)	Vertical Field-of-View:  3.6 to 10 mm: 54 to 26 degrees or 
8 to 18 mm: 46 to 27 degrees.
e)	Resolution:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
f)	Lens Focal Length:  3.6 to 10 mm or 8-18 mm varifocal.
g)	Current:  PoE:  0.27 A; 24 VAC:  0.55 A; 12 VDC:  1.1 A.
h)	Power Consumption IR and Heaters On:  16.5 W.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Digital Zoom:  Yes, ROI.
6)	Tilt and Horizontal:  Three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation.
7)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition.
8)	IR Distance:  Smart IR/Adaptive IR; 131 ft (40 m) with 22 IR LEDs.
f.	Physical Parameters:  
1)	Operating Temperature:  Minus 40 to 140 degrees F (Minus 40 to 60 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; polycarbonate clear dome. Dimensions:  4.49 in. (125 mm) x 5.3 in. (135 mm) diameter.
5)	Weight:  2.6 (1.2 kg). 
g.	Electrical Parameters:  
1)	Input Voltage:  24 VAC, 12 VDC or PoE.
2)	Connectors:  
a)	Two conduit access holes for internal cable termination.
b)	Power:  12 VDC or 24 VAC terminal block.
c)	PoE:  RJ-45.
d)	Video and Data:  RJ-45.
e)	Alarm:  Screw terminal.
f)	Audio:  Screw terminal, audio level alarm alert. 
g)	Slot for SD card.
h)	Composite output for installation-2-pin connector.
i)	Reset button.
j)	Default button.
3)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Frame Rate:  Up to 30 fps.
6)	Web Browser:  Safari, Firefox, Google Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. The cameras shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/M/T.
4.	Basis of Design:  V2105D Outdoor IP Dome Camera as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/M/T and NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Outdoor dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart IR capability.
3)	Intelligent Video Analysis, motion and tampering/defocus.
4)	Mounting:  Surface mountable. 
e.	Camera Parameters:
1)	Maximum Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  0.05 lux; Black and White:  0.03 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  96 to 32 degrees.
d)	Vertical Field-of-View:  69 to 24 degrees.
e)	Field-of-View Depth:  124 to 40 degrees.
f)	Resolution:  2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480.
2)	Shutter Speed:  1/2 - 1/10,000 sec.
3)	Automatic Gain Control:  On/Off selectable.
4)	Digital Zoom:  Yes, ROI.
5)	Tilt and Horizontal:  Two-direction adjustment, allowing for adjustment of pan and tilt.
6)	Lens Adjustment:  Motorized lens, DC-iris.
7)	IR Distance:  Smart IR; 98 ft (30 m) with 16 IR LEDs.
f.	Physical Parameters:  
1)	Operating Temperature:  Minus 22 to 140 degrees F (Minus 30 to 60 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; bracket:  PC+ABS; window:  double glass/polycarbonate clear dome. 
5)	Dimensions:  4.4 in. (112 mm) x 5.3 in. (135 mm) diameter.
6)	Weight:  2.2 (1 kg). 
g.	Electrical Parameters:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current:  PoE:  0.16 A; 12 VDC:  0.63 A.
3)	Power Consumption IR On:  7.6 W.
4)	Connectors:  
a)	Power:  12 VDC terminal block.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Slot for SD card.
e)	Reset button.
f)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Frame Rate:  Up to 30 fps.
6)	Web Browser:  Safari, Firefox, Google Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Tampering/Defocus, Motion.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
5.	Basis of Design:  V2360W-12-1 Outdoor IP Panoramic Dome Camera as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/M/T and NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Features:
1)	Outdoor panoramic dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart IR capability.
3)	Intelligent Video Analysis, motion and tampering/defocus.
4)	Mounting:  Surface mountable. 
e.	Camera Parameters:
1)	Imaging Device:  1/2.3 -inch.
2)	Maximum Resolution:  12 MP.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.07 lux; Black and White:  0.1 (IR OFF), 0 lux (IR On).
6)	Digital Zoom:  Dynamic ROI.
7)	Lens Adjustment:  Fixed fisheye.
8)	Focal Length:  1.6 mm.
9)	Field of View:  195 degrees, 360 degree surround view.
10)	IR Distance:  Smart IR; 49 ft (15 m) with 1 IR LED.
11)	Dual heater system.
f.	Physical Parameters:  
1)	Operating Temperature:  Minus 40 to 122 degrees F (Minus 40 to 50 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; bracket:  PC+ABS front case. 
5)	Dimensions:  2.2 in. (57 mm) x 5 in. (150 mm) diameter.
6)	Weight:  2 lb (0.9 kg). 
g.	Electrical Parameters:  
1)	Input Voltage:  24 VAC or PoE.
2)	Current:  PoE:  0.52 A; 24 VAC:  1.1 A.
3)	Power Consumption IR On:  13.9 W.
4)	Connectors:  
a)	Power:  24 VAC terminal block.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Audio In and Out:  Screw terminal; built-in mic; audio level alarm alert.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution:  2976x2976, 2592x2592, 2048x2048, 1952x1952, 1536x1536, 1280x1280, 960x960, 640x640
6)	Frame Rate:  Up to 30 fps.
7)	Web Browser:  Safari, Firefox, Google Chrome, Microsoft Edge.
8)	Users:  Live viewing for up to 10 clients.
9)	Image Settings:  Digital image effects defog, flip; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; dynamic ROI.
10)	Intelligent Video Analytics:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. It shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
11)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/M/T.
G.	Bullet Cameras:
1.	Basis of Design:  V2000B Outdoor IP Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	UL.
3)	FCC, Class A.
4)	IP67.
5)	IK10, including front glass.
6)	ONVIF S/T/G/M.
7)	RoHS.
8)	NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera; true WDR and Smart IR/Adaptive IR capability and include an integral varifocal DC-iris lens. 
4)	Motorized Lens:  Allow for remote configuration of zoom and focus (motorized focus and zoom). 
5)	Day/Night Operation:  Achieved using a built-in IR-cut filter.
6)	Camera Position:  Adjustable using the integral mount. Sunshield provided.
7)	Dual heater provided. 
8)	Triple streaming video and support H.264/H.265 and M-JPEG compression. 
9)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
e.	Day/Night IP Bullet Camera Specifications:
1)	Max. Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity at 30 IRE:  Color:  0.03 lux or 0.02 lux; 
black and white:  0.01 lux /0 lux (IR Off/On).
c)	Focal Length:  3.1 to 10 mm or 8-18 mm varifocal.
d)	Horizontal Field of View:  3.1 to 10 mm: 96 to 32 degrees or 
8 to 18 mm: 40 to 19 degrees.
e)	Vertical Field of View:  3.1 to 10 mm: 69 to 24 degrees or 
8 to 18 mm: 29 to 13 degrees.
f)	Current:  PoE:  0.42 A; 24 VAC:  0.83 A; 12 VDC:  1.67 A.
g)	Power Consumption, IR On:  20 W.
2)	Max. Resolution:  8 MP.
a)	Imaging Device:  1/1.8-inch progressive scan.
b)	Sensitivity at 30 IRE:  Color:  0.02 lux or 0.01 lux;
black and white:  0.01 lux /0 lux (IR Off/On).
c)	Focal Length:  3.6 to 10 mm or 8-18 mm varifocal.
d)	Horizontal Field of View:  3.6 to 10 mm: 98 to 46 degrees or 
8 to 18 mm:  60 to 25 degrees.
e)	Vertical Field of View:  3.6 to 10 mm: 54 to 26 degrees or 
8 to 18 mm: 33 to 12 degrees.
f)	Current:  PoE:  0.41 A; 24 VAC:  0.82 A; 12 VDC:  1.64 A.
g)	Power Consumption, IR On:  21.6 W.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Tilt and Horizontal:  Three-direction adjustment, allowing for adjustment of pan, tilt and rotation.
5)	Digital Zoom:  Yes (ROI).
6)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition.
7)	IR Distance:  Smart IR/Adaptive IR; 131 ft (40 m) with 4 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  24 VAC, 12 VDC or PoE Plus.
2)	Connectors:
a)	Power:  12 VDC or 24 VAC terminal block.
b)	PoE:  RJ-45.
c)	Video/Data:  RJ-45.
d)	Alarm:  Screw terminal.
e)	Audio:  Screw terminal.
f)	Slot for SD card.
g)	Reset button.
h)	Default button.
3)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 40 to 140 degrees F (minus 40 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum alloy body; sunshield:  PC+ABS.
4)	Dimensions:  
a)	Length:  10.3 inch (261 mm).
b)	Diameter:  3.5 inch (89 mm).
c)	Weight:  4 lbs (1.8 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  Integral mount allows positioning.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution, 5 MP:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
6)	Resolution, 8 MP:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
7)	Frame Rate:  Max 30 fps.
8)	Web Browser:  Safari, Firefox, Chrome, Microsoft Edge.
9)	Users:  Live viewing for up to 10 clients.
10)	Image Settings:  Digital image effects defog, flip and mirror; configurable, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
11)	Intelligent Video Analytics:  Intelligent Video Analytics:  Tampering, Intelligent Motion Detection, Intrusion Detection; Line Cross, Loitering, Object Left/Removed, Tailgating, Crowding. The cameras shall also provide AI-based object classification analytics for vehicles, people and animals. This shall enhance working with Museum Search in Valerus VMS.
12)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/M/T.
2.	Basis of Design:  V2105B Outdoor IP Bullet Camera as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	UL.
3)	FCC, Class A.
4)	IP67.
5)	IK08.
6)	ONVIF S/T/G/M.
7)	RoHS.
8)	NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 5-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera; true WDR and Smart IR capability and include an integral varifocal DC-iris lens. 
4)	Motorized Lens:  Allow for remote configuration of zoom and focus (motorized focus and zoom). 
5)	Day/Night Operation:  Achieved using a built-in IR-cut filter.
6)	Camera Position:  Adjustable using the integral mount. 
7)	Triple streaming video and support H.264/H.265 and M-JPEG compression. 
8)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
e.	Day/Night IP Bullet Camera Specifications:
1)	Imaging Device:  1/2.8-inch progressive scan.
2)	Maximum Resolution:  5 MP.
a)	Sensitivity at 30 IRE:  Color:  0.05 lux; 
black and white:  0.03 lux/0 lux (IR Off/On).
b)	Horizontal Field of View:  96 to 32 degrees.
c)	Vertical Field of View:  69 to 24 degrees.
d)	Depth Field of View:  124 to 40 degrees.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Tilt and Horizontal:  Two-direction adjustment, allowing for adjustment of pan and tilt.
6)	Digital Zoom:  Yes (ROI).
7)	Lens Adjustment:  Motorized lens, DC-iris.
8)	Focal Length:  3.1 to 10 mm varifocal.
9)	IR Distance:  Smart IR; 98 ft (30 m) with 16 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current:  PoE:  0.16 A; 12 VDC:  0.63 A.
3)	Power Consumption:  IR On:  7.6 W; IR Off:  5.2 W.
4)	Connectors:
a)	Pigtail cable provided.
b)	Power:  12 VDC terminal block.
c)	PoE:  RJ-45.
d)	Video/Data:  RJ-45.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 22 to 140 degrees F 
(minus 30 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum alloy body; bracket:  PC+ABS; 
window:  double glass/polycarbonate.
4)	Dimensions:  
a)	Length:  6.9 inch (177 mm).
b)	Width:  3.3 inch (84 mm).
c)	Height:  3.1 inch (79 mm).
d)	Weight:  2 lbs (0.9 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  2-axis camera adjustment.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution, 5 MP:  2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480.
6)	Frame Rate:  Max 30 fps.
7)	Web Browser:  Safari, Firefox, Chrome, Microsoft Edge.
8)	Users:  Live viewing for up to 10 clients.
9)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
10)	Video Content Analysis:  Tampering/defocus, motion.
11)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, DDNS, UDP, QoS, ARP, 

END OF SECTION